{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":57,"n_cols":12,"rows_kept":57,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBA-A(9)"]
[]
[]
[]
[]
["","","","","","FBA35A2VEB9","FBA50A2VEB9","FBA60A2VEB9","FBA71A2VEB9","FBA100A2VEB","FBA125A2VEB","FBA140A2VEB"]
["Dzesēšanas jauda","Kopējā jauda","","Nom.","kW","","","","","","14.00","15.40"]
["Apsildes jauda","Kopējā jauda","","Nom.","kW","","","","","","13.5","15.5"]
["Korpuss","Krāsa","","","","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)","Nav krāsots (galvanizēts)"]
["","Materiāls","","","","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne"]
["Izmēri","Ierīce","","Augstums","mm","245","245","245","245","245","245","245"]
["","","","Platums","mm","700","700","1000","1000","1400","1400","1400"]
["","","","Dziļums","mm","800","800","800","800","800","800","800"]
["Svars","Ierīce","","","kg","28.0","28.0","35.0","35.0","46.0","46.0","46.0"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","","Zema","m³/min.","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","","Apsilde","Augsta","m³/min.","15.0","15.0","18.0","18.0","29.0","34.0","34.0"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","12.5","12.5","15.0","15.0","24.5","29.0","29.0"]
["","","Apsilde","Zema","m³/min.","10.5","10.5","12.5","12.5","20.0","23.5","23.5"]
["","Ārējais statiskais spiediens","","Nom.","Pa","30","30","30","30","40","50","50"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","60.0","60.0","56.0","56.0","58.0","62.0","62.0"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","35.0","35.0","30.0","30.0","34.0","37.0","37.0"]
["","","","Vidēja","dBA","32.0","32.0","28.0","28.0","32.0","35.0","35.0"]
["","","","Zema","dBA","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["","Apsilde","","Augsta","dBA","37.0","37.0","31.0","31.0","36.0","38.0","38.0"]
["","","","Vidēja","dBA","34.0","34.0","28.0","28.0","33.0","35.0","35.0"]
["","","","Zema","dBA","29.0","29.0","25.0","25.0","30.0","32.0","32.0"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35","9.52","9.52","9.52","9.52"]
["","Gāze","","OD","mm","9.52","12.70","12.70","15.90","15.90","15.90","15.90"]
["","Aizplūde","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Novadīšanas augstums","mm","","","","625","625","625","625","625","625","625"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66","BRC4C65, BRC4C66"]
["","Tālv. pults ar vadu","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Installation manual","","","","1","1","1","","1","1","1"]
["","Washer for hanger bracket","","","","8","8","8","","8","8","8"]
["","Operation manual","","","","1","1","1","","1","1","1"]
["","Clamps","","","","4","4","4","","4","4","4"]
["","Drain hose","","","","1","1","1","","1","1","1"]
["","Insulation for fitting","","","","2","2","2","","2","2","2"]
["","Metal clamp for drain hose","","","","1","1","1","","1","1","1"]
["","Screws","","","","40","40","40","","40","40","40"]
["","Sealing pads","","","","5","5","5","","5","5","5"]
["Barošanas avots","Fāze","","","","1~","1~","1~","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50/60","50/60","50/60","50/60","50/60","50/60","50/60"]
["","Spriegums","","","V","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220","220-240/220"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","","","","1"]
["","Kronšteina skavas paplāksne","","","","","","","8"]
["","Lietošanas rokasgrāmata","","","","","","","1"]
["","Skavas","","","","","","","4"]
["","Izplūdes šļūtene","","","","","","","1"]
["","Piederumu izolācija","","","","","","","2"]
["","Izplūdes šļūtenes metāla skava","","","","","","","1"]
["","Skrūves","","","","","","","40"]
["","Blīvējuma paliktņi","","","","","","","5"]
["Notes","","","","","","","","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots."]
["","","","","","","","","(2) - Elektrības datus skatiet atsevišķā zīmējumā","","(2) - Elektrības datus skatiet atsevišķā zīmējumā"]