{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":13,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FBQ-D / RZQSG-L3/9V1"]
[]
[]
[]
[]
["","","","","FBQ35D2VEB / FBQ35D2VEB / RZQSG71L3V1B","FBQ100D2VEB / RZQSG100L9V1B","FBQ35D2VEB / FBQ35D2VEB / FBQ35D2VEB / RZQSG100L9V1B","FBQ50D2VEB / FBQ50D2VEB / RZQSG100L9V1B","FBQ125D2VEB / RZQSG125L9V1B","FBQ60D2VEB / FBQ60D2VEB / RZQSG125L9V1B","FBQ50D2VEB / FBQ50D2VEB / FBQ50D2VEB / RZQSG125L9V1B","FBQ140D2VEB / RZQSG140L9V1B","FBQ71D2VEB / RZQSG71L3V1B (Archived)"]
["Telpas dzesēšana","SEER","","","5.10","5.61","5.10","5.10","5.47","4.80","4.80"]
["","Gada enerģijas patēriņš","","kWh/a","467","593","652","652","768","875","875"]
["","Jauda","Pdesign","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00"]
["","Energoefektivitātes klase","","","A","A+","A","A","A","B","B"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","6.00","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","4.15","3.80","3.80","4.01","3.80","3.80"]
["","Energoefektivitātes klase","","","A","A+","A","A","A+","A","A"]
["","Gada enerģijas patēriņš","","kWh/a","2,211","2,564","2,800","2,800","2,653","2,800","2,800"]
["Notes","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]
["Dzesēšanas jauda","Nom.","","kW","","9.5 (2)","","","12.0 (2)","","","13.4 (2)"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","","1,418","","","1,858"]
["","EER","","","","3.35 (1)","","","3.23 (1)","","","3.06 (1)"]
["","COP","","","","3.67 (1)","","","3.63 (1)","","","3.40 (1)"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","A","","","A"]
["","","Apsilde","","","A","","","A"]
["Apsildes jauda","Nom.","","kW","","10.80 (2)","","","13.50 (2)","","","15.50 (2)"]
["Notes","","","","","(3) - Ikgadējais enerģijas patēriņš atbilst Energomarķējuma direktīvai 2002/31/EK","","","(3) - Ikgadējais enerģijas patēriņš atbilst Energomarķējuma direktīvai 2002/31/EK"]
["","","","","","(4) - SEER un SCOP atbilst EN 14825","","","(4) - SEER un SCOP atbilst EN 14825"]
["","","","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["Āra ierīce","","","","","","","","","","","","RZQSG71L3V1"]
["Dzesēšanas jauda","Nom.","","kW","","","","","","","","","6.8"]
["Apsildes jauda","Nom.","","kW","","","","","","","","","7.5"]
["Nominālā efektivitāte","EER","","","","","","","","","","","3.30"]
["","COP","","","","","","","","","","","3.81"]
["","Gada enerģijas patēriņš","","kWh","","","","","","","","","1030"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","","","","","","","","A"]
["","","Apsilde","","","","","","","","","","A"]
["Telpu dzesēšana","Energoefektivitātes klase","","","","","","","","","","","A+"]
["","Jauda","Pdesign","kW","","","","","","","","","6.80"]
["","SEER","","","","","","","","","","","5.84"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","","408"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","","","","","","","","","A+"]
["","Jauda","Pdesign","kW","","","","","","","","","6.00"]
["","SCOP/A","","","","","","","","","","","4.10"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","","2049"]