{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":36,"n_cols":18,"rows_kept":36,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FCAG100AVEB / RZQG100L8Y1B","FCAG125AVEB / RZQG125L8Y1B","FCAG50AVEB / FCAG50AVEB / FCAG50AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG100L8Y1B","FCAG60AVEB / FCAG60AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / RZQG71L8Y1B","FCAG71AVEB / RZQG71L8Y1B","FCAG50AVEB / FCAG50AVEB / RZQG71L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG100L8Y1B","FCAG71AVEB / FCAG71AVEB / RZQG125L8Y1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L7Y1B","FCAG140AVEB / RZQG140L7Y1B"]
["Dzesēšanas jauda","Nom.","","kW","","","","","","","","","6.80 (1)","","","","13.4 (1)","13.4 (1)"]
["Telpas dzesēšana","SEER","","","","","","","","","","5.10","6.72","5.10","","","9.70","6.44"]
["","ηs,c","","%","","","","","","","","","","","","","385.1","254.6"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","467","355","467","","","829","1,249"]
["","Jauda","Pdesign","kW","","","","","","","","6.80","6.80","6.80","","","13.4","13.4"]
["","Energoefektivitātes klase","","","","","","","","","","A","A++","A"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","","","","","","","","6.00","6.33","6.00","","","12.0","11.6"]
["","SCOP/A","","","","","","","","","","3.80","4.20","3.80","","","3.96","4.27"]
["","Energoefektivitātes klase","","","","","","","","","","A","A+","A"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","2,211","2,110","2,211","","","4,235","3,795"]
["","ηs,h","","%","","","","","","","","","","","","","155.2","167.6"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","","","","","","","","","1,005"]
["","EER","","","","","","","","","","","3.39 (3)","","","","4.29 (3)","2.50 (3)"]
["","COP","","","","","","","","","","","3.97 (3)","","","","","3.61 (3)"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","","","","","","","","A"]
["","","Apsilde","","","","","","","","","","A"]
["Apsildes jauda","Nom.","","kW","","","","","","","","","7.50 (2)","","","","15.5 (2)","15.5 (2)"]
["Notes","","","","","","","","","","","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m","","","","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m"]
["","","","","","","","","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5m; līmeņa atšķirība: 0 m","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5m; līmeņa atšķirība: 0 m","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5m; līmeņa atšķirība: 0 m","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5m; līmeņa atšķirība: 0 m"]
["","","","","","","","","","","","(3) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(3) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","","","(3) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(3) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["Energoefektivitātes diapazons","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","","","","A+++ ~ D","A+++ ~ D"]
["Āra ierīce","","","","","","","","","","","","","","RZQG100L8Y1","RZQG125L8Y1"]
["Telpu dzesēšana","Energoefektivitātes klase","","","","","","","","","","","","","A","A"]
["","Jauda","Pdesign","kW","","","","","","","","","","","9.50","12.0"]
["","SEER","","","","","","","","","","","","","5.10","5.10"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","","","","652","824"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","","","","","","","","","","","A","A"]
["","Jauda","Pdesign","kW","","","","","","","","","","","11.3","12.7"]
["","SCOP/A","","","","","","","","","","","","","3.80","3.80"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","","","","4164","4683"]