{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":11,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-A / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCAG50AVEB / FCAG50AVEB / RZQG71L9V1B","FCAG100AVEB / RZQG100L9V1B","FCAG140AVEB / RZQG100L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG100L9V1B","FCAG125AVEB / RZQG125L9V1B","FCAG71AVEB / FCAG71AVEB / RZQG125L9V1B","FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / FCAG35AVEB / RZQG140L9V1B"]
["Telpas dzesēšana","SEER","","","5.10","6.80","6.80","5.10","6.00","5.10","9.70"]
["","Gada enerģijas patēriņš","","kWh/a","467","489","489","652","700","824","829"]
["","Jauda","Pdesign","kW","6.80","9.50","9.50","9.50","12.0","12.0","13.4"]
["","Energoefektivitātes klase","","","A","A++","A++","A","A+","A"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","6.00","11.3","11.30","7.60","12.7","12.7","12.0"]
["","SCOP/A","","","3.80","4.61","4.61","3.80","4.10","3.80","3.96"]
["","Energoefektivitātes klase","","","A","A++","A++","A","A+","A"]
["","Gada enerģijas patēriņš","","kWh/a","2,211","3,432","3,432","4,164","4,323","4,683","4,235"]
["Dzesēšanas jauda","Nom.","","kW","","9.50 (1)","","","12.0 (1)","","13.4 (1)"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","","1,225","","","1,610"]
["","EER","","","","3.87 (3)","","","3.73 (3)","","4.29 (3)"]
["","COP","","","","4.15 (3)","","","3.63 (3)"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","A","","","A"]
["","","Apsilde","","","A","","","A"]
["Apsildes jauda","Nom.","","kW","","10.8 (2)","","","13.5 (2)","","15.5 (2)"]
["Notes","","","","","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m","","","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m","","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 7,5m; līmeņa atšķirība: 0 m"]
["","","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5m; līmeņa atšķirība: 0 m","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5m; līmeņa atšķirība: 0 m","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5m; līmeņa atšķirība: 0 m"]
["","","","","","(3) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","","(3) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","(3) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["Telpas dzesēšana","ηs,c","","%","","","","","","","385.1"]
["Telpu apsilde (mērens klimats)","ηs,h","","%","","","","","","","155.2"]