{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":20,"n_cols":6,"rows_kept":20,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAG-B / RXS-L"]
[]
[]
[]
[]
["","","","","FCAG50BVEB / RXS50L2V1B","FCAG60BVEB / RXS60L2V1B"]
["Dzesēšanas jauda","Nom.","","kW","5.00","5.70"]
["Apsildes jauda","Nom.","","kW","6.00","7.00"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","705","820"]
["","COP","","","3.70","3.52"]
["","EER","","","3.55","3.48"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","A"]
["","","Apsilde","","A","B"]
["Cauruļu savienojumi","Izplūde","OD","mm","VP25 (Ārējais diametrs 32, iekšējais diametrs 25)","VP25 (Ārējais diametrs 32, iekšējais diametrs 25)"]
["","Gāze","OD","mm","12.70","12.70"]
["","Šķidrums","OD","mm","6.35","6.35"]
["Notes","","","","(1) - Normālas darbības apstākļos: +22°C / + 32°C","(1) - Normālas darbības apstākļos: +22°C / + 32°C"]
["","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]