{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":5,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCAHG-G / RZAG-NV1"]
[]
[]
[]
[]
["","","","","FCAHG100GVEB / RZAG100N7V1B"]
["Dzesēšanas jauda","Nom.","","kW","9.50 (1)"]
["Apsildes jauda","Nom.","","kW","10.8 (2)"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A++"]
["","Jauda","Pdesign","kW","9.50"]
["","SEER","","","7.35"]
["","Gada enerģijas patēriņš","","kWh/a","452"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A++"]
["","Jauda","Pdesign","kW","9.52"]
["","SCOP/A","","","4.81"]
["","Gada enerģijas patēriņš","","kWh/a","2,771"]
["Notes","","","","(1) - Dzesēšana: T2: iekštelpu temp. 26,6°CDB, 19,4°CWB, āra temp. 48°CDB [Btu/hr/W]"]
["","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]