{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":13,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F / RZQG-L9V1"]
[]
[]
[]
[]
["","","","","FCQHG71FVEB / RZQG71L9V1B","FCQHG100FVEB / RZQG71L9V1B","FCQHG100FVEB / RZQG100L9V1B","FCQHG140FVEB / RZQG100L9V1B","FCQHG71FVEB / FCQHG71FVEB / RZQG100L9V1B","FCQHG125FVEB / RZQG125L9V1B","FCQHG140FVEB / RZQG125L9V1B","FCQHG71FVEB / FCQHG71FVEB / RZQG125L9V1B","FCQHG140FVEB / RZQG140L9V1B"]
["Dzesēšanas jauda","Nom.","","kW","6.8","","9.5","","","12.0","","","13.4"]
["Space cooling","SEER","","","6.91","7.00","7.00","7.00","5.10","6.61","6.61","5.10"]
["","Gada enerģijas patēriņš","","kWh/a","345","340","475","475","652","636","636","824"]
["","Jauda","Pdesign","kW","6.80","6.80","9.50","9.50","9.50","12.00","12.00","12.00"]
["","Energoefektivitātes klase","","","A++","A++","A++","A++","B","A++","A++","B"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","7.60","7.60","11.30","11.30","11.30","12.66","12.66","12.71"]
["","SCOP/A","","","4.54","4.54","4.80","4.80","3.80","4.63","4.63","3.80"]
["","Energoefektivitātes klase","","","A+","A+","A++","A++","A","A++","A++","A"]
["","Gada enerģijas patēriņš","","kWh/a","2,344","2,344","3,296","3,296","4,164","3,829","3,829","4,683"]
["Nominālā efektivitāte","Annual energy consumption","","kWh","830","","1,075","","","1,500"]
["","EER","","","4.09","","4.42","","","4.00","","","3.35"]
["","COP","","","4.80","","4.99","","","4.40","","","4.12"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","","A","","","A"]
["","","Apsilde","","A","","A","","","A"]
["Apsildes jauda","Nom.","","kW","7.5","","10.8","","","13.5","","","15.5"]
["Notes","","","","(1) - Ikgadējais enerģijas patēriņš atbilst Energomarķējuma direktīvai 2002/31/EK","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - SEER un SCOP atbilst EN 14825","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]