{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":117,"n_cols":9,"rows_kept":117,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FCQHG-F"]
[]
[]
[]
[]
["","","","","","FCQHG71FVEB","FCQHG100FVEB","FCQHG125FVEB","FCQHG140FVEB"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["","","","Zema","dBA","","33","35","37"]
["","Dzesēšana","","Zema","dBA","","33","35","37"]
["","","","Augsta","dBA","","44","45","45"]
["","","","Nom.","dBA","","39","40","41"]
["Standard Accessories","Lietošanas rokasgrāmata","","","","","Lietošanas rokasgrāmata","Lietošanas rokasgrāmata","Lietošanas rokasgrāmata"]
["","Uzstādīšanas rokasgrāmata","","","","","Uzstādīšanas rokasgrāmata","Uzstādīšanas rokasgrāmata","Uzstādīšanas rokasgrāmata"]
["","Izplūdes šļūtene","","","","","Izplūdes šļūtene","Izplūdes šļūtene","Izplūdes šļūtene"]
["","Izplūdes šļūtenes skava","","","","","Izplūdes šļūtenes skava","Izplūdes šļūtenes skava","Izplūdes šļūtenes skava"]
["","Kronšteina skavas paplāksne","","","","","Kronšteina skavas paplāksne","Kronšteina skavas paplāksne","Kronšteina skavas paplāksne"]
["","Skrūves","","","","","Skrūves","Skrūves","Skrūves"]
["","Uzstādīšanas ceļvedis","","","","","Uzstādīšanas ceļvedis","Uzstādīšanas ceļvedis","Uzstādīšanas ceļvedis"]
["","Piederumu izolācija","","","","","2","2","2"]
["","Blīvējuma paliktņi","","","","","4","4","4"]
["","Drenāžas blīvējuma paliktnis","","","","","Drenāžas blīvējuma paliktnis","Drenāžas blīvējuma paliktnis","Drenāžas blīvējuma paliktnis"]
["","Skavas","","","","","Skavas","Skavas","Skavas"]
["Vadības sistēmas","Wired remote control","","","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","","","BRC7FA532F","BRC7FA532F","BRC7FA532F"]
["Piping connections","Šķidrums","","OD","mm","","9.52","9.52","9.52"]
["","Gāze","","OD","mm","","15.9","15.9","15.9"]
["","Aizplūde","","","","","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)","VP25 (I.D. 25/O.D. 32)"]
["Apdares panelis 4","Izmēri","","Dziļums","mm","","50","50","50"]
["","","","Platums","mm","","950","950","950"]
["","","","Augstums","mm","","950","950","950"]
["","Modelis","","","","","BYCQ140D7W1 - balts ar pelēkām žalūzijām","BYCQ140D7W1 - balts ar pelēkām žalūzijām","BYCQ140D7W1 - balts ar pelēkām žalūzijām"]
["","Krāsa","","","","","Dzidri balts (RAL 9010)","Dzidri balts (RAL 9010)","Dzidri balts (RAL 9010)"]
["","Svars","","","kg","","5.4","5.4","5.4"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","61","61","61"]
["","Apsilde","","","dBA","","61","61","61"]
["Izmēri","Ierīce","","Platums","mm","","840","840","840"]
["","","","Dziļums","mm","","840","840","840"]
["","","","Augstums","mm","","288","288","288"]
["Korpuss","Materiāls","","","","","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne"]
["Svars","Ierīce","","","kg","","26","26","26"]
["Apdares panelis","Svars","","","kg","","10.3","10.3","10.3"]
["","Modelis","","","","","BYCQ140D7GFW1 - automātiski attīrošais panelis ar smalka sieta filtru","BYCQ140D7GFW1 - automātiski attīrošais panelis ar smalka sieta filtru","BYCQ140D7GFW1 - automātiski attīrošais panelis ar smalka sieta filtru"]
["","Izmēri","","Augstums","mm","","130","130","130"]
["","","","Dziļums","mm","","950","950","950"]
["","","","Platums","mm","","950","950","950"]
["","Krāsa","","","","","Tīri balts (RAL 9010)","Tīri balts (RAL 9010)","Tīri balts (RAL 9010)"]
["Power supply","Phase","","","","","1~","1~","1~"]
["","Frekvence","","","Hz","","50","50","50"]
["","Nosaukums","","","","","VE","VE","VE"]
["","Spriegums","","","V","","220-240","220-240","220-240"]
["Notes","","","","","","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots."]
["","","","","","","(2) - BYCQ140D7W1W ir balta izolācija. Netīrumu veidošanās uz baltas izolācijas ir labāk redzama, tāpēc BYCQ140D7W1W apdares paneli nav ieteicams uzstādīt vietā, kur iespējama netīrumu koncentrācija.","(2) - BYCQ140D7W1W ir balta izolācija. Netīrumu veidošanās uz baltas izolācijas ir labāk redzama, tāpēc BYCQ140D7W1W apdares paneli nav ieteicams uzstādīt vietā, kur iespējama netīrumu koncentrācija.","(2) - BYCQ140D7W1W ir balta izolācija. Netīrumu veidošanās uz baltas izolācijas ir labāk redzama, tāpēc BYCQ140D7W1W apdares paneli nav ieteicams uzstādīt vietā, kur iespējama netīrumu koncentrācija."]
["","","","","","","(3) - BYCQ140D7W1: dzidri balts standarta panelis ar pelēkām žalūzijām; BYCQ140D7W1W: dzidri balts standarta panelis ar baltām žalūzijām; BYCQ140D7GW1: dzidri palts panelis ar automātiskās tīrīšanas funkciju.","(3) - BYCQ140D7W1: dzidri balts standarta panelis ar pelēkām žalūzijām; BYCQ140D7W1W: dzidri balts standarta panelis ar baltām žalūzijām; BYCQ140D7GW1: dzidri palts panelis ar automātiskās tīrīšanas funkciju.","(3) - BYCQ140D7W1: dzidri balts standarta panelis ar pelēkām žalūzijām; BYCQ140D7W1W: dzidri balts standarta panelis ar baltām žalūzijām; BYCQ140D7GW1: dzidri palts panelis ar automātiskās tīrīšanas funkciju."]
["Korpuss","Materiāls","","","","Galvanizēta tērauda plāksne"]
["Izmēri","Ierīce","","Augstums","mm","288"]
["","","","Platums","mm","840"]
["","","","Dziļums","mm","840"]
["Svars","Ierīce","","","kg","25"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","21.2"]
["","","","Nom.","m³/min.","16.7"]
["","","","Zema","m³/min.","12.2"]
["","","Apsilde","Augsta","m³/min.","21.2"]
["","","","Nom.","m³/min.","16.7"]
["","","","Zema","m³/min.","12.2"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","53"]
["","Apsilde","","","dBA","53"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Zema","dBA","29"]
["","Apsilde","","Augsta","dBA","36"]
["","","","Nom.","dBA","33"]
["","","","Zema","dBA","29"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","9.52"]
["","Gāze","","OD","mm","15.9"]
["","Aizplūde","","","","VP25 (I.D. 25/O.D. 32)"]
["Apdares panelis","Modelis","","","","BYCQ140D7GFW1 - automātiski attīrošais panelis ar smalka sieta filtru"]
["","Krāsa","","","","Tīri balts (RAL 9010)"]
["","Izmēri","","Augstums","mm","130"]
["","","","Platums","mm","950"]
["","","","Dziļums","mm","950"]
["","Svars","","","kg","10.3"]
["Apdares panelis 2","Modelis","","","","BYCQ140D7GW1 - panelis ar automātisko attīrīšanās funkciju"]
["","Krāsa","","","","Tīri balts (RAL 9010)"]
["","Izmēri","","Augstums","mm","130"]
["","","","Platums","mm","950"]
["","","","Dziļums","mm","950"]
["","Svars","","","kg","10.3"]
["Apdares panelis 3","Modelis","","","","BYCQ140D7W1W - pilnīgi balta"]
["","Krāsa","","","","Tīri balts (RAL 9010)"]
["","Izmēri","","Augstums","mm","50"]
["","","","Platums","mm","950"]
["","","","Dziļums","mm","950"]
["","Svars","","","kg","5.4"]
["Apdares panelis 4","Modelis","","","","BYCQ140D7W1 - balta ar pelēkām žalūzijām"]
["","Krāsa","","","","Tīri balts (RAL 9010)"]
["","Izmēri","","Augstums","mm","950"]
["","","","Platums","mm","950"]
["","","","Dziļums","mm","50"]
["","Svars","","","kg","5.4"]
["Vadības sistēmas","Infrared remote control","","","","BRC7FA532F"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","BRC1D52, BRC1E52A/B"]
["Standard Accessories","Installation manual","","","","Installation manual"]
["","Washer for hanger bracket","","","","Washer for hanger bracket"]
["","Operation manual","","","","Operation manual"]
["","Clamp for drain hose","","","","Clamp for drain hose"]
["","Clamps","","","","Clamps"]
["","Drain hose","","","","Drain hose"]
["","Drain sealing pad","","","","Drain sealing pad"]
["","Installation guide","","","","Installation guide"]
["","Insulation for fitting","","","","2"]
["","Screws","","","","Screws"]
["","Sealing pads","","","","4"]
["Barošanas avots","Nosaukums","","","","VE"]
["","Fāze","","","","1~"]
["Strāvas padeve","Strāvas padeve-=-Frekvence","","Frekvence","","50"]
["","Strāvas padeve-=-Spriegums","","Spriegums","","220-240"]