{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":67,"n_cols":8,"rows_kept":67,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDA-A"]
[]
[]
[]
[]
["","","","","","FDA125A5VEB","FDA200AXVEB","FDA250AXVEB"]
["Dzesēšanas jauda","Kopējā jauda","","Nom.","kW","12.10","19.00","22.00"]
["Apsildes jauda","Kopējā jauda","","Nom.","kW","13.50","22.4","24.0"]
["Korpuss","Krāsa","","","","Nekrāsots","Nekrāsots","Nekrāsots"]
["","Materiāls","","","","Galvanizēts tērauds","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne"]
["Izmēri","Ierīce","","Augstums","mm","300","470","470"]
["","","","Platums","mm","1,400","1,490","1,490"]
["","","","Dziļums","mm","700","1,100","1,100"]
["Svars","Ierīce","","","kg","45","104","115"]
["Nepieciešamais griestu atstatums >","mm","","","","350"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","39.0","64.0","69.0"]
["","","","Vidēja","m³/min.","","50","56"]
["","","","Zema","m³/min.","28.0","36.0","43.0"]
["","","Apsilde","Augsta","m³/min.","39.0","64.0","69.0"]
["","","","Vidēja","m³/min.","","50.0","56.0"]
["","","","Zema","m³/min.","28.0","36.0","43.0"]
["","Ārējais statiskais spiediens","","Augsts","Pa","200","250","250"]
["","","","Nom.","Pa","50","62","62"]
["Sound power level","Dzesēšana","","","dBA","66","69.0","71.0"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","40","43.0","44.0"]
["","","","Vidēja","dBA","","39.0","40.0"]
["","","","Zema","dBA","33","36.0","37.0"]
["","Apsilde","","Augsta","dBA","40","43.0","44.0"]
["","","","Vidēja","dBA","","39.0","40.0"]
["","","","Zema","dBA","33","36.0","37.0"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","9.52","9.52","9.52"]
["","Gāze","","OD","mm","15.90","19.1","22.2"]
["","Izplūde","","","","VP25 (I.D. 25/O.D. 32)","BSP1","BSP1"]
["Novadīšanas augstums","mm","","","","625"]
["Apdares panelis","Modelis","","","","BYBS125DJW1"]
["","Krāsa","","","","Balts (10Y9/0,5)"]
["","Izmēri","","Augstums","mm","55"]
["","","","Platums","mm","1,500"]
["","","","Dziļums","mm","500"]
["","Svars","","","kg","6.5"]
["Vadības sistēmas","Infrared remote control","","","","BRC4C65, BRC4C66"]
["","Tālv. pults ar vadu","","","","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52","BRC1H52W/S/K, BRC1E53A, BRC1E53B, BRC1E53C, BRC1D52"]
["Standard Accessories","Lietošanas rokasgrāmata","","","","","1","1"]
["","Uzstādīšanas un lietošanas rokasgrāmata","","","","1","1","1"]
["","Uzstādīšanas rokasgrāmata","","","","","1","1"]
["","Vispārēji drošības pasākumi","","","","1","1","1"]
["","Gāzes savienojuma cauruļvads","","","","","1","1"]
["","Vadu skavas materiāls","","","","","1","1"]
["","Paplāksne","","","","8","12","12"]
["","Atsperpaplāksne","","","","","2","2"]
["","Skrūve + paplāksne","","","","","45","45"]
["","Skrūve ar sešstūru galvu un plaplāksni","","","","","49","49"]
["","Skrūves","","","","16","2","2"]
["","Skrūve ar sešstūru galvu","","","","","2","2"]
["","Plakanā paplāksne","","","","","8","8"]
["Power supply","Nosaukums","","","","","VE","VE"]
["","Fāze","","","","1~","1~","1~"]
["","Frekvence","","","Hz","50/60","50/60","50/60"]
["","Spriegums","","","V","220-240/220","220-240/220","220-240/220"]
["Standard Accessories","Šļūtenes apkava","","","","1"]
["","Izplūdes šļūtene","","","","1"]
["","Vads kopējai elektroapgādei","","","","2"]
["","Blīvējošais materiāls (noliešanas caurule)","","","","1"]
["","Blīvējamais materiāls","","","","2"]
["","Termoizolācijas caurule (šķidrums)","","","","1"]
["","Termoizolācijas caurule (gāze)","","","","1"]
["Notes","","","","","(1) - Elektrības datus skatiet atsevišķā zīmējumā"]