{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":37,"n_cols":7,"rows_kept":37,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDBQ-B"]
[]
[]
[]
[]
["","","","","","FDBQ25B5V1","FDBQ25B8V1"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","35.0","35.0"]
["","","","Zema","dBA","29.0","29.0"]
["","Dzesēšana","","Zema","dBA","28.0","28.0"]
["","","","Augsta","dBA","35.0","35.0"]
["Standard Accessories","Uzstādīšanas un lietošanas rokasgrāmata","","","","1","1"]
["","Izsūkšanas gaisa filtrs","","","","1","1"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","BRC1D52, BRC1E52A/B"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35"]
["","Gāze","","OD","mm","9.52"]
["","Izplūde","","","","27.2"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","55","55"]
["","Apsilde","","","dBA","55","55"]
["Izmēri","Ierīce","","Platums","mm","652","652"]
["","","","Dziļums","mm","502","502"]
["","","","Augstums","mm","230","230"]
["Korpuss","Materiāls","","","","Tērauds ar nelielu oglekļa sastāvu un cinka pārklājumu","Tērauds ar nelielu oglekļa sastāvu un cinka pārklājumu"]
["Svars","Ierīce","","","kg","17.0","17.0"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","","6.95"]
["","","","Zema","m³/min.","","5.20"]
["","","Dzesēšana","Zema","m³/min.","","5.20"]
["","","","Augsta","m³/min.","","6.50"]
["Power supply","Fāze","","","","1~","1~"]
["","Frekvence","","","Hz","50","50"]
["","Nosaukums","","","","V1","V1"]
["","Spriegums","","","V","230","230 +/-10%"]
["Notes","","","","","(1) - Skaņas vērtības tiek mērītas pusatbalsojošā nodalījumā.","(1) - Skaņas vērtības tiek mērītas pusatbalsojošā nodalījumā."]
["","","","","","(2) - Skaņas spiediena līmenis ir relatīva vērtība atbilstoši atstatumam un akustiskajai videi. Papildinformāciju, lūdzu, skatiet skaņas līmeņa zīmējumos.","(2) - Skaņas spiediena līmenis ir relatīva vērtība atbilstoši atstatumam un akustiskajai videi. Papildinformāciju, lūdzu, skatiet skaņas līmeņa zīmējumos."]
["","","","","","(3) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(3) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots."]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","6.35"]
["","Gāze","","OD","mm","","9.52"]
["","Izplūde","","","","","27.2"]