{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":22,"n_cols":5,"rows_kept":22,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDQ-B / RZQ-D3/D9V1"]
[]
[]
[]
[]
["","","","","FDQ125B8V3B9 / RZQ125D9V1B"]
["Dzesēšanas jauda","Nom.","","kW","12.5 (3)"]
["Cauruļvadu savienojumi","Šķidrums","OD","mm","9.52"]
["","Gāze","OD","mm","15.9"]
["","Drain","OD","mm","26"]
["Telpas dzesēšana","SEER","","","3.50"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","1,978"]
["","EER","","","3.16"]
["","COP","","","3.88"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","B"]
["","","Apsilde","","A"]
["Apsildes jauda","Nom.","","kW","14.0 (4)"]
["Notes","","","","(1) - Enerģijas uzlīme: skalā no A (visefektīvākā) līdz G (visneefektīvākā)"]
["","","","","(2) - Gada enerģijas patēriņš: pamatojoties uz vidējo izmantojumu 500 darba stundās gadā ar pilnu slodzi (nominālos apstākļos)"]
["","","","","(3) - Dzesēšana: iekšējo temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 5m; līmeņa atšķirība: 0 m"]
["","","","","(4) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5m; līmeņa atšķirība: 0 m"]
["","","","","(5) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]