{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":14,"n_cols":9,"rows_kept":14,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F / 2MXM-M"]
[]
[]
[]
[]
["","","","","FDXM25F2V1B / FDXM50F2V1B / 2MXM50M2V1B","FDXM25F2V1B / FDXM25F2V1B / 2MXM50M2V1B","FDXM25F2V1B / FDXM35F2V1B / 2MXM50M2V1B","FDXM35F2V1B / FDXM50F2V1B / 2MXM50M2V1B","FDXM35F2V1B / FDXM35F2V1B / 2MXM50M2V1B"]
["Dzesēšanas jauda","Nom.","","kW","5.00","5.00","5.00","5.00","5.00"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","713","780","770","704","761"]
["","EER","","","3.51","3.21","3.25","3.55","3.29"]
["","COP","","","3.61","3.66","3.64","3.61","3.62"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","A","A","A","A"]
["","","Apsilde","","A","A","A","A","A"]
["Apsildes jauda","Min.","","kW","5.60","5.60","5.60","5.60","5.60"]
["Notes","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]