{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":28,"n_cols":6,"rows_kept":28,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXM50F3V1B / RXS50L2V1B","FDXM60F3V1B / RXS60L2V1B"]
["Dzesēšanas jauda","Nom.","","kW","5.00","6.00"]
["Telpas dzesēšana","SEER","","","5.72","5.51"]
["","Gada enerģijas patēriņš","","kWh/a","306","381"]
["","Jauda","Pdesign","kW","5.00","6.00"]
["","Energoefektivitātes klase","","","A+","A"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","4.00","4.60"]
["","SCOP/A","","","3.93","3.80"]
["","Energoefektivitātes klase","","","A","A"]
["","Gada enerģijas patēriņš","","kWh/a","1,425","1,693"]
["Cauruļvadu savienojumi","Šķidrums","OD","mm","6.35","6.35"]
["","Gāze","OD","mm","12.70","12.70"]
["","Izplūde","OD","mm","VP20 (Ārējais diametrs 26, iekšējais diametrs 20)","VP20 (Ārējais diametrs 26, iekšējais diametrs 20)"]
["Nominālā efektivitāte","EER","","","3.03","2.91"]
["","Gada enerģijas patēriņš","","kWh","825","1,030"]
["","COP","","","3.10","3.21"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","B","C"]
["","","Apsilde","","D","C"]
["Apsildes jauda","Nom.","","kW","5.80","7.00"]
["Notes","","","","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]