{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":11,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F3 / RZAG-MY1"]
[]
[]
[]
[]
["","","","","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG71M7Y1B","FDXM35F3V1B / FDXM35F3V1B / RZAG71M7Y1B","FDXM50F3V1B / FDXM50F3V1B / RZAG71M7Y1B","FDXM50F3V1B / FDXM50F3V1B / FDXM50F3V1B / RZAG100M7Y1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7Y1B","FDXM35F3V1B / FDXM35F3V1B / FDXM35F3V1B / RZAG100M7Y1B","FDXM50F3V1B / FDXM50F3V1B / RZAG100M7Y1B"]
["Dzesēšanas jauda","Nom.","","kW","6.80 (1)","6.80 (1)","6.80 (1)","9.50 (1)","9.50 (1)","9.50 (1)","9.50 (1)"]
["Telpu dzesēšana","Gada enerģijas patēriņš","","kWh/a","377","380","334","379","416","423","387"]
["","Jauda","Pdesign","kW","6.80","6.80","6.80","9.50","9.50","9.50","9.50"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","4.70","4.70","4.70","7.80","7.80","7.80","7.80"]
["","Gada enerģijas patēriņš","","kWh/a","1,537","1,589","1,485","2,324","2,438","2,540","2,421"]
["Apsildes jauda","Nom.","","kW","7.50 (2)","7.50 (2)","7.50 (2)","10.8 (2)","10.8 (2)","10.8 (2)","10.8 (2)"]
["Telpu dzesēšana","SEER","","","6.32","6.27","7.12","8.77","8.00","7.86","8.60"]
["","Energoefektivitātes klase","","","A++","A++","A++","A+++","A++","A++","A+++"]
["Telpu apsilde (mērens klimats)","SCOP/A","","","4.28","4.14","4.43","4.70","4.48","4.30","4.51"]
["","Energoefektivitātes klase","","","A+","A+","A+","A++","A+","A+","A+"]
["Notes","","","","(1) - Dzesēšana: iekšējo temp. 27°CDB, 19°CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 5m; līmeņa atšķirība: 0 m","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","","","","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]