{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":9,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXM-F9"]
[]
[]
[]
[]
["","","","","","FDXM25F3V1B9","FDXM35F3V1B9","FDXM50F3V1B9","FDXM60F3V1B9"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","35.0","35.0","","38.0"]
["","","","Vidēja","dBA","33.0","33.0","","35.0"]
["","","","Zema","dBA","27.0","27.0","","30.0"]
["","Dzesēšana","","Vidēja","dBA","33.0","33.0","","35.0"]
["","","","Zema","dBA","27.0","27.0","","30.0"]
["","","","Augsta","dBA","35.0","35.0","","38.0"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","1","","1"]
["","Lietošanas rokasgrāmata","","","","1","1","","1"]
["","Piederumu izolācija","","","","1","1","","1"]
["","Blīvējuma paliktnis","","","","1","1","","1"]
["","Metāla skava","","","","1","1","","1"]
["","Izplūdes šļūtene","","","","1","1","","1"]
["","Kronšteina skavas paplāksne","","","","8","8","","8"]
["","Blīvējamais materiāls","","","","2","2","","2"]
["","Skavas","","","","6","6","","6"]
["","Paplāksnes fiksācijas plāksne","","","","4","4","","4"]
["","Cauruļu uzmalu skrūves","","","","1","1","","1"]
["","Gaisa filtrs","","","","1","1","","1"]
["Piping connections","Šķidrums","","OD","mm","6.35","6.35","","6.35"]
["","Gāze","","OD","mm","9.50","9.50","","12.70"]
["","Izplūde","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","","VP20 (I.D. 20/O.D. 26)"]
["Jaudas izlietojums","Dzesēšana","","Nom.","kW","0.036","0.036","","0.060"]
["","Apsilde","","Nom.","kW","0.036","0.036","","0.060"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","53.0","53.0","","56.0"]
["","Apsilde","","","dBA","53.0","53.0","","56.0"]
["Izmēri","Ierīce","","Platums","mm","750","750","","1,150"]
["","","","Dziļums","mm","620","620","","620"]
["","","","Augstums","mm","200","200","","200"]
["Svars","Ierīce","","","kg","21","21","","28"]
["Ventilators","Ārējais statiskais spiediens","","Nom.","Pa","30","30","","40"]
["","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","8.7","8.7","","16.0"]
["","","","Vidēja","m³/min.","8.0","8.0","","14.8"]
["","","","Zema","m³/min.","7.3","7.3","","13.5"]
["","","Dzesēšana","Zema","m³/min.","7.3","7.3","","13.5"]
["","","","Vidēja","m³/min.","8.0","8.0","","14.8"]
["","","","Augsta","m³/min.","8.7","8.7","","16.0"]
["Power supply","Fāze","","","","1~","1~","","1~"]
["","Frekvence","","","Hz","50","50","","50"]
["","Spriegums","","","V","220-240","220-240","","220-240"]
["Notes","","","","","(1) - Elektrības datus skatiet atsevišķā zīmējumā","(1) - Elektrības datus skatiet atsevišķā zīmējumā","","(1) - Elektrības datus skatiet atsevišķā zīmējumā"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","","","0.060"]
["","Apsilde","","Nom.","kW","","","0.060"]
["Izmēri","Ierīce","","Augstums","mm","","","200"]
["","","","Platums","mm","","","1150"]
["","","","Dziļums","mm","","","620"]
["Svars","Ierīce","","","kg","","","28"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","","15.8"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","","14.6"]
["","","","Zema","m³/min.","","","13.3"]
["","","Apsilde","Augsta","m³/min.","","","15.8"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","","","14.6"]
["","","Apsilde","Zema","m³/min.","","","13.3"]
["","Ārējais statiskais spiediens","","Nom.","Pa","","","40"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","","55.0"]
["","Apsilde","","","dBA","","","55.0"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","","38.0"]
["","","","Vidēja","dBA","","","35.0"]
["","","","Zema","dBA","","","30.0"]
["","Apsilde","","Augsta","dBA","","","38.0"]
["","","","Vidēja","dBA","","","35.0"]
["","","","Zema","dBA","","","30.0"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","","6.35"]
["","Gāze","","OD","mm","","","12.70"]
["","Aizplūde","","","","","","VP20 (I.D. 20/O.D. 26)"]
["Standard Accessories","Installation manual","","","","","","1"]
["","Washer for hanger bracket","","","","","","8"]
["","Operation manual","","","","","","1"]
["","Clamp metal","","","","","","1"]
["","Clamps","","","","","","6"]
["","Drain hose","","","","","","1"]
["","Gaisa filtrs","","","","","","1"]
["","Insulation for fitting","","","","","","1"]
["","Screws for duct flanges","","","","","","1"]
["","Sealing material","","","","","","2"]
["","Sealing pad","","","","","","1"]
["","Washer fixing plate","","","","","","4"]
["Barošanas avots","Fāze","","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","","50"]
["","Spriegums","","","V","","","220-240"]