{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-C / RXS-F"]
[]
[]
[]
[]
["","","","","FDXS60CVMB / RXS60F3V1B"]
["Cooling capacity","Min.","","kW","1.7"]
["","Maks.","","kW","6.5"]
["","Nom.","","kW","6.0 (1)"]
["Cauruļvadu savienojumi","Liquid","OD","mm","6.35"]
["","Gāze","OD","mm","12.7"]
["","Izplūde","OD","mm","26"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","1,065"]
["","EER","","","2.82"]
["","COP","","","3.02"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","C"]
["","","Apsilde","","D"]
["Apsildes jauda","Nom.","","kW","7.0 (2)"]
["","Min.","","kW","1.7"]
["","Maks.","","kW","8.0"]
["Notes","","","","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 7,5 m"]
["","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 7,5 m"]
["","","","","(3) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]