{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":21,"n_cols":5,"rows_kept":21,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-E / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS25E7VMB / RXS25K2V1B"]
["Dzesēšanas jauda","Nom.","","kW","2.40 (3)"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35"]
["","Gāze","OD","mm","9.5"]
["","Izplūde","OD","mm","VP20 (Ārējais diametrs 26, iekšējais diametrs 20)"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","345"]
["","EER","","","3.48"]
["","COP","","","3.52"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A"]
["","","Apsilde","","B"]
["Apsildes jauda","Nom.","","kW","3.20 (4)"]
["Notes","","","","(1) - Enerģijas uzlīme: skalā no A (visefektīvākā) līdz G (visneefektīvākā)"]
["","","","","(2) - Gada enerģijas patēriņš: pamatojoties uz vidējo izmantojumu 500 darba stundās gadā ar pilnu slodzi (nominālos apstākļos)"]
["","","","","(3) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35°CDB; ekvivalentais cauruļvadu garums: 5m; līmeņa atšķirība: 0 m"]
["","","","","(4) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5m; līmeņa atšķirība: 0 m"]
["","","","","(5) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]