{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":6,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RXS-K"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / RXS35K2V1B","FDXS50F2VEB / RXS50K2V1B"]
["Dzesēšanas jauda","Min.","","kW","1.4","1.7"]
["","Maks.","","kW","3.8","5.3"]
["","Nom.","","kW","3.4 (2)","5.0 (2)"]
["Cauruļvadu savienojumi","Šķidrums","OD","mm","6.35","6.35"]
["","Gāze","OD","mm","9.5","12.7"]
["","Izplūde","OD","mm","VP20 (Ārējais diametrs 26, iekšējais diametrs 20)","VP20 (Ārējais diametrs 26, iekšējais diametrs 20)"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","530","825"]
["","EER","","","3.21 (1)","3.03 (1)"]
["","COP","","","3.39 (1)","3.10 (1)"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","B"]
["","","Apsilde","","C","D"]
["Apsildes jauda","Nom.","","kW","4.0 (3)","5.8 (3)"]
["","Min.","","kW","1.4","1.7"]
["","Maks.","","kW","5.0","6.0"]
["Notes","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m","(2) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m"]
["","","","","(3) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m","(3) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m"]
["","","","","(4) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(4) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]