{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":17,"n_cols":10,"rows_kept":17,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F / RZQSG-L(3/8)V1"]
[]
[]
[]
[]
["","","","","FDXS35F2VEB / FDXS35F2VEB / RZQSG71L3V1B","FDXS50F2VEB / FDXS50F2VEB / RZQSG100L8V1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQSG100L8V1B","FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / FDXS35F2VEB / RZQSG125L8V1B","FDXS50F2VEB / FDXS50F2VEB / FDXS50F2VEB / RZQSG125L8V1B","FDXS60F2VEB / FDXS60F2VEB / RZQSG125L8V1B"]
["Telpu dzesēšana","SEER","","","5.10","5.10","5.10","4.80","4.80","4.80"]
["","Gada enerģijas patēriņš","","kWh/a","467","652","652","875","875","875"]
["","Jauda","Pdesign","kW","6.80","9.50","9.50","12.00","12.00","12.00"]
["","Energoefektivitātes klase","","","A","A","A","B","B","B"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","6.00","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","3.80","3.80","3.80","3.80","3.80"]
["","Energoefektivitātes klase","","","A","A","A","A","A","A"]
["","Gada enerģijas patēriņš","","kWh/a","2,211","2,800","2,800","2,800","2,800","2,800"]
["Notes","","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]