{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":23,"n_cols":5,"rows_kept":23,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9 / RXS-L"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9 / RXS50L2V1B"]
["Dzesēšanas jauda","Min.","","kW","1.7"]
["","Maks.","","kW","5.3"]
["","Nom.","","kW","5.0"]
["Cauruļvadu savienojumi","Šķidrums","OD","mm","6.35"]
["","Gāze","OD","mm","12.7"]
["","Izplūde","OD","mm","VP20 (Ārējais diametrs 26, iekšējais diametrs 20)"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","825"]
["","EER","","","3.03"]
["","COP","","","3.10"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","B"]
["","","Apsilde","","D"]
["Apsildes jauda","Nom.","","kW","5.8"]
["","Min.","","kW","1.7"]
["","Maks.","","kW","6.0"]
["Notes","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - 230 V"]
["","","","","(3) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]