{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FDXS-F9"]
[]
[]
[]
[]
["","","","","FDXS50F2VEB9"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","38"]
["","","Vidēja","dBA","36"]
["","","Zema","dBA","30"]
["","Dzesēšana","Vidēja","dBA","36"]
["","","Zema","dBA","30"]
["","","Augsta","dBA","38"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","1"]
["","Lietošanas rokasgrāmata","","","1"]
["","Piederumu izolācija","","","1"]
["","Blīvējuma paliktnis","","","1"]
["","Metāla skava","","","1"]
["","Izplūdes šļūtene","","","1"]
["","Kronšteina skavas paplāksne","","","8"]
["","Blīvējamais materiāls","","","2"]
["","Skavas","","","6"]
["","Paplāksnes fiksācijas plāksne","","","4"]
["","Cauruļu uzmalu skrūves","","","1"]
["","Gaisa filtrs","","","1"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35"]
["","Gāze","OD","mm","12.7"]
["","Izplūde","","","VP20 (I.D. 20/O.D. 26)"]
["Power input","Dzesēšana","Nom.","kW","0.060"]
["","Apsilde","Nom.","kW","0.060"]
["Sound power level","Dzesēšana","","dBA","55"]
["","Apsilde","","dBA","55"]
["Izmēri","Ierīce","Platums","mm","1,150"]
["","","Dziļums","mm","620"]
["","","Augstums","mm","200"]
["Svars","Ierīce","","kg","30.0"]
["Ventilators","Ārējais statiskais spiediens","Nom.","Pa","40"]
["Power supply","Fāze","","","1~"]
["","Frekvence","","Hz","50/60"]
["","Nosaukums","","","VE"]
["","Spriegums","","V","220-240"]
["Notes","","","","(1) - Savienojot ar multisistēmas āra ierīci, skatiet pievienojamās āra multiierīces tehniskos datus."]