{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A / RXM-N"]
[]
[]
[]
[]
["","","","","FFA50A2VEB / RXM50N2V1B","FFA60A2VEB / RXM60N2V1B"]
["Dzesēšanas jauda","Nom.","","kW","","5.70"]
["Apsildes jauda","Nom.","","kW","","7.00"]
["Nominālā efektivitāte","EER","","","","3.05"]
["","COP","","","","3.41"]
["","Gada enerģijas patēriņš","","kWh","","934"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","B"]
["","","Apsilde","","","B"]
["Telpu dzesēšana","Energoefektivitātes klase","","","","A+"]
["","Jauda","Pdesign","kW","","5.70"]
["","SEER","","","","5.76"]
["","Gada enerģijas patēriņš","","kWh/a","","347"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","","A+"]
["","Jauda","Pdesign","kW","","3.96"]
["","SCOP/A","","","","4.04"]
["","Gada enerģijas patēriņš","","kWh/a","","1,372"]
["Notes","","","","","(1) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","(2) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","","(3) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","","(4) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["Outdoor unit","","","","RXM50N2V1B"]
["Dzesēšanas jauda","Nom.","","kW","5.00"]
["Apsildes jauda","Nom.","","kW","5.80"]
["Nominālā efektivitāte","EER","","","3.24"]
["","COP","","","3.49"]
["","Gada enerģijas patēriņš","","kWh","771"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A"]
["","","Apsilde","","B"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A+"]
["","Jauda","Pdesign","kW","5.00"]
["","SEER","","","5.98"]
["","Gada enerģijas patēriņš","","kWh/a","292"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A"]
["","Jauda","Pdesign","kW","3.84"]
["","SCOP/A","","","3.90"]
["","Pdh Apsildes jauda pie -10°","","kW","3.51"]
["","Gada enerģijas patēriņš","","kWh/a","1377"]
["Energoefektivitātes diapazons","","","","A+++ ~ D"]