{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":64,"n_cols":9,"rows_kept":64,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FFA-A"]
[]
[]
[]
[]
["","","","","","FFA25A2VEB","FFA35A2VEB","FFA50A2VEB","FFA60A2VEB"]
["Korpuss","Materiāls","","","","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne"]
["Izmēri","Ierīce","","Augstums","mm","260","260","260","260"]
["","","","Platums","mm","575","575","575","575"]
["","","","Dziļums","mm","575","575","575","575"]
["Svars","Ierīce","","","kg","16.0","16.0","17.5","17.5"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","9.0","10.0","12.0","14.5"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","8.0","8.5","10.0","12.5"]
["","","","Zema","m³/min.","6.5","6.5","7.5","9.5"]
["","","Apsilde","Augsta","m³/min.","9.0","10.0","12.0","14.5"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","8.0","8.5","10.0","12.5"]
["","","Apsilde","Zema","m³/min.","6.5","6.5","7.5","9.5"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","48","51","56","60"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","31.0","34.0","39.0","43.0"]
["","","","Vidēja","dBA","28.5","30.5","34.0","40.0"]
["","","","Zema","dBA","25.0","25.0","27.0","32.0"]
["","Apsilde","","Augsta","dBA","31.0","34.0","39.0","43.0"]
["","","","Vidēja","dBA","28.5","30.5","34.0","40.0"]
["","","","Zema","dBA","25.0","25.0","27.0","32.0"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35","6.35"]
["","Gāze","","OD","mm","9.52","9.52","12.70","12.70"]
["","Aizplūde","","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Apdares panelis","Modelis","","","","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W","BYFQ60C2W1W"]
["","Krāsa","","","","Balts (N9.5)","Balts (N9.5)","Balts (N9.5)","Balts (N9.5)"]
["","Izmēri","","Augstums","mm","46","46","46","46"]
["","","","Platums","mm","620","620","620","620"]
["","","","Dziļums","mm","620","620","620","620"]
["","Svars","","","kg","2.8","2.8","2.8","2.8"]
["Apdares panelis 2","Modelis","","","","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S","BYFQ60C2W1S"]
["","Krāsa","","","","Sudraba","Sudraba","Sudraba","Sudraba"]
["","Izmēri","","Augstums","mm","46","46","46","46"]
["","","","Platums","mm","620","620","620","620"]
["","","","Dziļums","mm","620","620","620","620"]
["","Svars","","","kg","2.8","2.8","2.8","2.8"]
["Apdares panelis 3","Modelis","","","","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1","BYFQ60B2W1"]
["","Krāsa","","","","White (RAL9010)","White (RAL9010)","White (RAL9010)","White (RAL9010)"]
["","Izmēri","","Augstums","mm","55","55","55","55"]
["","","","Platums","mm","700","700","700","700"]
["","","","Dziļums","mm","700","700","700","700"]
["","Svars","","","kg","2.7","2.7","2.7","2.7"]
["Apdares panelis 4","Modelis","","","","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1","BYFQ60B3W1"]
["","Krāsa","","","","White (RAL9010)","White (RAL9010)","White (RAL9010)","White (RAL9010)"]
["","Izmēri","","Augstums","mm","55","55","55","55"]
["","","","Platums","mm","700","700","700","700"]
["","","","Dziļums","mm","700","700","700","700"]
["","Svars","","","kg","2.7","2.7","2.7","2.7"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","BRC7EB530 (standarta panelis), BRC7F530W (balts panelis), BRC7F530S (pelēks panelis)","BRC7EB530 (standarta panelis), BRC7F530W (balts panelis), BRC7F530S (pelēks panelis)","BRC7EB530 (standarta panelis), BRC7F530W (balts panelis), BRC7F530S (pelēks panelis)","BRC7EB530 (standarta panelis), BRC7F530W (balts panelis), BRC7F530S (pelēks panelis)"]
["","Tālv. pults ar vadu","","","","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7","BRC1D528, BRC1E53A7, BRC1E53B7, BRC1E53C7"]
["Standard Accessories","Washer for hanger bracket","","","","8","8","8","8"]
["","Thermal insulation tube","","","","2","2","2","2"]
["","Hose band","","","","1","1","1","1"]
["","Drain hose","","","","1","1","1","1"]
["","Installation and operation manual","","","","1","1","1","1"]
["","Screws","","","","4","4","4","4"]
["","Sealing material","","","","4","4","4","4"]
["","Tie-wraps","","","","7","7","7","7"]
["Barošanas avots","Fāze","","","","1~","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50","50","50"]
["","Spriegums","","","V","220-240","220-240","220-240","220-240"]