{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":26,"n_cols":5,"rows_kept":26,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A(9) / RXM-A8"]
[]
[]
[]
[]
["","","","","FHA50AVEB98 / RXM50A5V1B8"]
["Dzesēšanas jauda","Nom.","","kW","5"]
["Apsildes jauda","Nom.","","kW","6"]
["Nominālā efektivitāte","EER","","","3.1"]
["","COP","","","3.23"]
["","Gada enerģijas patēriņš","","kWh","806"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","B"]
["","","Apsilde","","C"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A+"]
["","Jauda","Pdesign","kW","5"]
["","SEER","","","5.84"]
["","Gada enerģijas patēriņš","","kWh/a","300"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A"]
["","Jauda","Pdesign","kW","4.35"]
["","SCOP/A","","","3.82"]
["","Pdh Apsildes jauda pie -10°","","kW","3.55"]
["","Gada enerģijas patēriņš","","kWh/a","1594"]
["Notes","","","","(1) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["","","","","(2) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]