{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":42,"n_cols":7,"rows_kept":42,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A / RXM-M9"]
[]
[]
[]
[]
["","","","","FHA35AVEB / RXM35M3V1B9","FHA50AVEB / RXM50M3V1B9","FHA60AVEB / RXM60M3V1B9"]
["Dzesēšanas jauda","Nom.","","kW","3.40"]
["Telpas dzesēšana","SEER","","","6.24"]
["","Gada enerģijas patēriņš","","kWh/a","191"]
["","Jauda","Pdesign","kW","3.40"]
["","Energoefektivitātes klase","","","A++"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","3.10"]
["","SCOP/A","","","4.43"]
["","Energoefektivitātes klase","","","A+"]
["","Gada enerģijas patēriņš","","kWh/a","979"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","456"]
["","EER","","","3.73"]
["","COP","","","4.08"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A"]
["","","Apsilde","","A"]
["Apsildes jauda","Nom.","","kW","4.00"]
["Notes","","","","(1) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","(2) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(3) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","(4) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["Āra ierīce","","","","","RXM50M3V1B9","RXM60M3V1B9"]
["Dzesēšanas jauda","Nom.","","kW","","5.00","5.70"]
["Apsildes jauda","Nom.","","kW","","6.00","7.20"]
["Nominālā efektivitāte","EER","","","","3.21","3.29"]
["","COP","","","","3.35","3.32"]
["","Gada enerģijas patēriņš","","kWh","","780","867"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","B","A"]
["","","Apsilde","","","C","C"]
["Telpu dzesēšana","Energoefektivitātes klase","","","","A+","A+"]
["","Jauda","Pdesign","kW","","5.00","5.70"]
["","SEER","","","","5.92","6.08"]
["","Gada enerģijas patēriņš","","kWh/a","","295","328"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","","A","A"]
["","Jauda","Pdesign","kW","","4.35","4.71"]
["","SCOP/A","","","","3.86","3.87"]
["","Pdh Apsildes jauda pie -10°","","kW","","3.85","4.08"]
["","Gada enerģijas patēriņš","","kWh/a","","1578","1704"]