{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":8,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHA-A"]
[]
[]
[]
[]
["","","","","FHA35AVEB","FHA50AVEB","FHA60AVEB","FHA71AVEB"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","36","37","37","38"]
["","","Nom.","dBA","34","35","35","36"]
["","","Vidēja","dBA","31","32","33","34"]
["","Dzesēšana","Vidēja","dBA","34","35","35","36"]
["","","Zema","dBA","31","32","33","34"]
["","","Augsta","dBA","36","37","37","38"]
["Standard Accessories","Termiskās izolācijas caurule","","","2","2","2","2"]
["","Vadu skavas materiāls","","","7","7","7","7"]
["","Šļūtenes apkava","","","1","1","1","1"]
["","Izplūdes šļūtene","","","1","1","1","1"]
["","Paplāksne","","","8","8","8","8"]
["","Blīvējuma paliktnis (liels)","","","1","1","1","1"]
["","Blīvējuma paliktnis (mazs)","","","1","1","1","1"]
["","Epoksīda sveķu iemava","","","1","1","1","1"]
["","Skrūves","","","2","2","2","2"]
["","Vadu stiprinājumi","","","2","2","2","2"]
["Vadības sistēmas","Tālv. pults ar vadu","","","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7","BRC1E53A7, BRC1E53B7, BRC1E53C7, BRC1D528, BRC1E51A7"]
["","Infrared remote control","","","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56","BRC7GA53, BRC7GA56"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35","6.35","6.35","9.52"]
["","Gāze","OD","mm","9.50","12.7","12.7","15.9"]
["","Izplūde","","","VP20","VP20","VP20","VP20"]
["Skaņas jaudas līmenis","Dzesēšana","","dBA","53","54","54","55"]
["Izmēri","Ierīce","Platums","mm","960","960","1,270","1,270"]
["","","Dziļums","mm","690","690","690","690"]
["","","Augstums","mm","235","235","235","235"]
["Korpuss","Materiāls","","","Sveķi, lokšņu metāls","Sveķi, lokšņu metāls","Sveķi, lokšņu metāls","Sveķi, lokšņu metāls"]
["","Krāsa","","","Balts","Balts","Balts","Balts"]
["Svars","Ierīce","","kg","24.0","25.0","31.0","32.0"]
["Power supply","Fāze","","","1~","1~","1~","1~"]
["","Frekvence","","Hz","50","50","50","50"]
["","Spriegums","","V","220-240","220-240","220-240","220-240"]
["Notes","","","","(1) - Elektrības datus skatiet atsevišķā zīmējumā","(1) - Elektrības datus skatiet atsevišķā zīmējumā","(1) - Elektrības datus skatiet atsevišķā zīmējumā","(1) - Elektrības datus skatiet atsevišķā zīmējumā"]