{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":32,"n_cols":12,"rows_kept":32,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQG-L(8)Y1"]
[]
[]
[]
[]
["","","","","FHQ71CAVEB / RZQG71L8Y1B","FHQ100CAVEB / RZQG71L8Y1B","FHQ100CAVEB / RZQG100L8Y1B","FHQ140CAVEB / RZQG100L8Y1B","FHQ140CAVEB / RZQG125L8Y1B","FHQ125CAVEB / RZQG125L8Y1B","FHQ140CAVEB / RZQG140L7Y1B","FHQ71CAVEB / FHQ71CAVEB / RZQG125L8Y1B (Archived)"]
["Dzesēšanas jauda","Nom.","","kW","6.8","","9.5","","","12.0","13.4"]
["Telpas dzesēšana","SEER","","","6.95","6.95","6.11","6.11","6.01","6.01"]
["","Gada enerģijas patēriņš","","kWh/a","343","343","545","545","699","699"]
["","Jauda","Pdesign","kW","6.8","6.80","9.5","9.50","12.00","12"]
["","Energoefektivitātes klase","","","A++","A++","A++","A++","A+","A+"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","7.6","7.60","11.3","11.30","14.13","14.13"]
["","SCOP/A","","","4.32","4.32","4.61","4.61","4.23","4.23"]
["","Energoefektivitātes klase","","","A+","A+","A++","A++","A+","A+"]
["","Gada enerģijas patēriņš","","kWh/a","2,463","2,463","3,432","3,432","4,677","4,677"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","890","","1,245","","","1,790"]
["","EER","","","3.82","","3.81","","","3.35","3.31"]
["","COP","","","4.13","","4.15","","","3.89","3.63"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","","A","","","A"]
["","","Apsilde","","A","","A","","","A"]
["Apsildes jauda","Nom.","","kW","7.5","","10.8","","","13.5","15.5"]
["Notes","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]
["Outdoor unit","","","","","","","","","","","RZQG125L8Y1"]
["Telpu dzesēšana","Energoefektivitātes klase","","","","","","","","","","B"]
["","Jauda","Pdesign","kW","","","","","","","","12.00"]
["","SEER","","","","","","","","","","5.10"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","824"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","","","","","","","","A"]
["","Jauda","Pdesign","kW","","","","","","","","12.71"]
["","SCOP/A","","","","","","","","","","3.80"]
["","Gada enerģijas patēriņš","","kWh/a","","","","","","","","4683"]