{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":24,"n_cols":13,"rows_kept":24,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FHQ-C / RZQSG-L(3/8)V1"]
[]
[]
[]
[]
["","","","","FHQ35CAVEB / FHQ35CAVEB / RZQSG71L3V1B","FHQ100CAVEB / RZQSG100L8V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG100L8V1B","FHQ50CAVEB / FHQ50CAVEB / RZQSG100L8V1B","FHQ125CAVEB / RZQSG125L8V1B","FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / FHQ35CAVEB / RZQSG125L8V1B","FHQ50CAVEB / FHQ50CAVEB / FHQ50CAVEB / RZQSG125L8V1B","FHQ60CAVEB / FHQ60CAVEB / RZQSG125L8V1B","FHQ140CAVEB / RZQSG140L7V1B"]
["Dzesēšanas jauda","Nom.","","kW","","9.5","","","12.0","","","","13.4"]
["Telpu dzesēšana","SEER","","","5.10","5.61","5.10","5.10","5.61","4.80","4.80","4.80"]
["","Gada enerģijas patēriņš","","kWh/a","467","592.692","652","652","748.663","875","875","875"]
["","Jauda","Pdesign","kW","6.80","9.50","9.50","9.50","12.00","12.00","12.00","12.00"]
["","Energoefektivitātes klase","","","A","A+","A","A","A+","B","B","B"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","6.00","7.60","7.60","7.60","7.60","7.60","7.60","7.60"]
["","SCOP/A","","","3.80","3.91","3.80","3.80","4.01","3.80","3.80","3.80"]
["","Energoefektivitātes klase","","","A","A","A","A","A+","A","A","A"]
["","Gada enerģijas patēriņš","","kWh/a","2,211","2,721.228","2,800","2,800","2,653.367","2,800","2,800","2,800"]
["Nominālā efektivitāte","Annual energy consumption","","kWh","","1,480","","","2,075"]
["","EER","","","","3.21","","","2.89","","","","3.01"]
["","COP","","","","3.61","","","3.62","","","","3.41"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","A","","","C"]
["","","Apsilde","","","A","","","A"]
["Apsildes jauda","Nom.","","kW","","10.8","","","13.5","","","","15.5"]
["Notes","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]
["","","","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]