{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":44,"n_cols":5,"rows_kept":44,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FLXS-B9"]
[]
[]
[]
[]
["","","","","FLXS35BAVMB9"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","46"]
["","","Klusa darbība","dBA","30"]
["","","Zema","dBA","33"]
["","Dzesēšana","Klusa darbība","dBA","29"]
["","","Zema","dBA","32"]
["","","Augsta","dBA","38"]
["","","Nom.","dBA","36"]
["","Dzesēšana","Nom.","dBA","35"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","1"]
["","Lietošanas rokasgrāmata","","","1"]
["","Infrasarkanā tālvadība","","","1"]
["","AAA sausās baterijas","","","2"]
["","Tālvadības turētājs","","","1"]
["","Montāžas plāksne","","","1"]
["","Siltumizolācijas caurule (dzesētāja cauruļvads)","","","8"]
["","Gaisa attīrīšanas filtrs","","","1"]
["","Fotokatalītiskais dezodorējošais filtrs","","","1"]
["","Malas pārsegs","","","2"]
["","Saistošā apmale","","","4"]
["Vadības sistēmas","Infrared remote control","","","ARC433B67"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35"]
["","Gāze","OD","mm","9.5"]
["","Izplūde","","","18"]
["Skaņas jaudas līmenis","Dzesēšana","","dBA","53"]
["","Apsilde","","dBA","59"]
["Izmēri","Ierīce","Platums","mm","1,050"]
["","","Dziļums","mm","200"]
["","","Augstums","mm","490"]
["Korpuss","Colour","","","Mandeļu balts"]
["Svars","Ierīce","","kg","16"]
["Power supply","Fāze","","","1~"]
["","Frekvence","","Hz","50"]
["","Nosaukums","","","VM"]
["","Spriegums","","V","220-240"]
["Notes","","","","(1) - 220 V"]
["","","","","(2) - 230 V"]
["","","","","(3) - 240 V"]
["","","","","(4) - Savienojot ar multisistēmas āra ierīci, skatiet pievienojamās āra multiierīces tehniskos datus."]