{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":6,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNA-A9 / RXM-R9"]
[]
[]
[]
[]
["","","","","FNA25A2VEB9 / RXM25R5V1B9","FNA35A2VEB9 / RXM35R5V1B9"]
["Dzesēšanas jauda","Nom.","","kW","2.60","3.40"]
["Apsildes jauda","Nom.","","kW","3.20","4.00"]
["Nominālā efektivitāte","EER","","","3.80","3.09"]
["","COP","","","4.00","3.48"]
["","Gada enerģijas patēriņš","","kWh","342","550"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","B"]
["","","Apsilde","","A","B"]
["Telpas dzesēšana","Energoefektivitātes klase","","","","A+"]
["","Jauda","Pdesign","kW","","3.40"]
["","SEER","","","","5.70"]
["","Gada enerģijas patēriņš","","kWh/a","","209"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","","A+"]
["","Jauda","Pdesign","kW","","2.90"]
["","SCOP/A","","","","4.05"]
["","Gada enerģijas patēriņš","","kWh/a","","1,002"]
["Notes","","","","(1) - Elektrības datus skatiet atsevišķā zīmējumā","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","(2) - Darbības diapazonu skatiet atsevišķā attēlā","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["","","","","(3) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(4) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]