{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":34,"n_cols":8,"rows_kept":34,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FNQ-A"]
[]
[]
[]
[]
["","","","","FNQ25A2VEB","FNQ35A2VEB","FNQ50A2VEB","FNQ60A2VEB"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","33","33","36","36"]
["","","Nom.","dBA","31","31","33","33"]
["","","Zema","dBA","28","28","30","30"]
["","Dzesēšana","Zema","dBA","28","28","30","30"]
["","","Augsta","dBA","33","33","36","36"]
["","","Nom.","dBA","31","31","33","33"]
["Refrigerant","GWP","","","2,087.5","2,087.5","2,087.5","2,087.5"]
["Vadības sistēmas","Tālv. pults ar vadu","","","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B","BRC1D52, BRC1E52A/B"]
["","Infrared remote control","","","BRC4C65","BRC4C65","BRC4C65","BRC4C65"]
["Dzesēšanas jauda","Kopējā jauda","Nom.","kW","2.6","3.4","5.0","6.0"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35","6.35","6.35","6.35"]
["","Gāze","OD","mm","9.52","9.52","12.7","12.7"]
["","Drain","","","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)","VP20 (I.D. 20/O.D. 26)"]
["Skaņas jaudas līmenis","Dzesēšana","","dBA","53","53","56","56"]
["Izmēri","Ierīce","Platums","mm","790","790","1,190","1,190"]
["","","Dziļums","mm","200","200","200","200"]
["","","Augstums","mm","620, 720 (2)","620, 720 (2)","620, 720 (2)","620, 720 (2)"]
["Korpuss","Materiāls","","","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne","Galvanizēta tērauda plāksne"]
["","Krāsa","","","Nekrāsots","Nekrāsots","Nekrāsots","Nekrāsots"]
["Svars","Ierīce","","kg","23","23","30","30"]
["Ventilators","Ārējais statiskais spiediens","Augsts","Pa","48","48","49","49"]
["","","Nom.","Pa","30","30","40","40"]
["Apsildes jauda","Kopējā jauda","Nom.","kW","3.2","4.0","5.8","7.0"]
["Power supply","Fāze","","","1~","1~","1~","1~"]
["","Frekvence","","Hz","50/60","50/60","50/60","50/60"]
["","Spriegums","","V","220-240/220","220-240/220","220-240/220","220-240/220"]
["Notes","","","","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots.","(1) - Skaņas jaudas līmenis ir absolūta vērtība, kas apzīmē jaudu, kuru ģenerē skaņas avots."]
["","","","","(2) - Ietver uzstādīšanai paredzētās kājas","(2) - Ietver uzstādīšanai paredzētās kājas","(2) - Ietver uzstādīšanai paredzētās kājas","(2) - Ietver uzstādīšanai paredzētās kājas"]