{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":92,"n_cols":10,"rows_kept":92,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXA-AW"]
[]
[]
[]
[]
["","","","","","FTXA20A2V1BW","FTXA25A2V1BW","FTXA35A2V1BW","FTXA42A2V1BW","FTXA50A2V1BW"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","39","40","41","","46"]
["","","","Vidēja","dBA","32","33","33","","42"]
["","","","Klusa darbība","dBA","19","19","19","","24"]
["","","","Zema","dBA","25","25","25","","33"]
["","Dzesēšana","","Vidēja","dBA","32","33","33","","39"]
["","","","Klusa darbība","dBA","19","19","19","","24"]
["","","","Zema","dBA","25","25","25","","31"]
["","","","Augsta","dBA","39","40","41","","46"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","1","1","","1"]
["","Lietošanas rokasgrāmata","","","","1","1","1","","1"]
["","Gaisa filtrs","","","","2","2","2","","2"]
["","Infrasarkanā tālvadība","","","","1","1","1","","1"]
["","Attālā kontrollera montāžas plāksne","","","","1","1","1","","1"]
["","Skrūvju somiņa","","","","1","1","1","","1"]
["","Skrūvju pārsegs","","","","1","1","1","","1"]
["","AAA sausās baterijas","","","","2","2","2","","2"]
["","Vispārēji drošības pasākumi","","","","1","1","1","","1"]
["Refrigerant","GWP","","","","675.0","675.0","675.0","","675.0"]
["Vadības sistēmas","Wired remote control","","","","BRC073","BRC073","BRC073","","BRC073"]
["","Infrared remote control","","","","ARC466A58","ARC466A58","ARC466A58","","ARC466A58"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35","","6.35"]
["","Gāze","","OD","mm","9.50","9.50","9.50","","12.70"]
["","Izplūde","","","","18","18","18","","18"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.020","0.022","0.023","","0.030"]
["","Apsilde","","Nom.","kW","0.020","0.020","0.022","","0.039"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","57","57","60","","60"]
["Izmēri","Ierīce","","Platums","mm","798","798","798","","798"]
["","","","Dziļums","mm","189","189","189","","189"]
["","","","Augstums","mm","295","295","295","","295"]
["Korpuss","Colour","","","","Balts","Balts","Balts","","Balts"]
["Svars","Ierīce","","","kg","11.50","11.50","11.50","","11.50"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","10.9","11.1","11.5","","15.1"]
["","","","Vidēja","m³/min.","8.7","9.0","9.0","","11.1"]
["","","","Zema","m³/min.","6.4","6.4","6.4","","8.2"]
["","","","Klusa darbība","m³/min.","4.5","4.5","4.5","","5.7"]
["","","Dzesēšana","Zema","m³/min.","6.1","6.1","6.1","","7.6"]
["","","","Vidēja","m³/min.","8.2","8.6","8.6","","10.4"]
["","","","Augsta","m³/min.","11.0","11.5","11.9","","13.5"]
["","","","Klusa darbība","m³/min.","4.6","4.6","4.6","","5.2"]
["Power supply","Fāze","","","","1~","1~","1~","","1~"]
["","Nosaukums","","","","V1","V1","V1","","V1"]
["","Frekvence","","","Hz","50","50","50","","50"]
["","Spriegums","","","V","220-240","220-240","220-240","","220-240"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","","","","0.028"]
["","Apsilde","","Nom.","kW","","","","0.036"]
["Korpuss","Krāsa","","","","","","","Balts"]
["Izmēri","Ierīce","","Augstums","mm","","","","295"]
["","","","Platums","mm","","","","798"]
["","","","Dziļums","mm","","","","189"]
["Svars","Ierīce","","","kg","","","","11.50"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","","","13.1"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","","","9.8"]
["","","","Zema","m³/min.","","","","7.2"]
["","","","Klusa darbība","m³/min.","","","","4.6"]
["","","Apsilde","Augsta","m³/min.","","","","14.6"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","","","","10.5"]
["","","Apsilde","Zema","m³/min.","","","","7.7"]
["","","","Klusa darbība","m³/min.","","","","5.2"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","","","60"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","","","45"]
["","","","Vidēja","dBA","","","","37"]
["","","","Zema","dBA","","","","29"]
["","","","Klusa darbība","dBA","","","","21"]
["","Apsilde","","Augsta","dBA","","","","45"]
["","","","Vidēja","dBA","","","","37"]
["","","","Zema","dBA","","","","29"]
["","","","Klusa darbība","dBA","","","","21"]
["Aukstumaģents","GWP","","","","","","","675.0"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","","","6.35"]
["","Gāze","","OD","mm","","","","12.70"]
["","Aizplūde","","","","","","","18"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","","","","ARC466A58"]
["","Tālv. pults ar vadu","","","","","","","BRC073"]
["Standard Accessories","Installation manual","","","","","","","1"]
["","Screw cover","","","","","","","1"]
["","AAA dry-cell batteries","","","","","","","2"]
["","General safety precautions","","","","","","","1"]
["","Operation manual","","","","","","","1"]
["","Gaisa filtrs","","","","","","","2"]
["","Infrared remote control","","","","","","","1"]
["","Remote controller mounting plate","","","","","","","1"]
["","Screw bag","","","","","","","1"]
["Barošanas avots","Nosaukums","","","","","","","V1"]
["","Fāze","","","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","","","50"]
["","Spriegums","","","V","","","","220-240"]