{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":38,"n_cols":6,"rows_kept":38,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXF-B"]
[]
[]
[]
[]
["","","","","FTXF20B5V1B","FTXF25B5V1B"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","39","40"]
["","","Vidēja","dBA","34","34"]
["","","Klusa darbība","dBA","21","21"]
["","","Zema","dBA","28","28"]
["","Dzesēšana","Vidēja","dBA","33","33"]
["","","Klusa darbība","dBA","20","20"]
["","","Zema","dBA","25","26"]
["","","Augsta","dBA","39","40"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","1","1"]
["","Lietošanas rokasgrāmata","","","1","1"]
["","Infrasarkanā tālvadība","","","1","1"]
["","AAA sausās baterijas","","","2","2"]
["","Tālvadības turētājs","","","1","1"]
["","Montāžas plāksne","","","1","1"]
["","Iekštelpu ierīces fiksācijas skrūves","","","2","2"]
["Control systems","Wired remote control","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["","Infrared remote control","","","ARC470A1","ARC470A1"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35","6.35"]
["","Gāze","OD","mm","9.50","9.50"]
["","Izplūde","","","18","18"]
["Strāvas ievade","Dzesēšana","Nom.","kW","0.017","0.019"]
["","Apsilde","Nom.","kW","0.020","0.020"]
["Skaņas jaudas līmenis","Dzesēšana","","dBA","55","55"]
["","Apsilde","","dBA","55","55"]
["Izmēri","Ierīce","Platums","mm","770","770"]
["","","Dziļums","mm","225","225"]
["","","Augstums","mm","286","286"]
["Korpuss","Colour","","","Balts","Balts"]
["Svars","Ierīce","","kg","8.50","8.50"]
["Power supply","Fāze","","","1~","1~"]
["","Frekvence","","Hz","50","50"]
["","Spriegums","","V","220-240","220-240"]