{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":35,"n_cols":8,"rows_kept":35,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-AB / RXJ-M9"]
[]
[]
[]
[]
["","","","","FTXJ20A2V1BB / RXJ20M5V1B9","FTXJ25A2V1BB / RXJ25M5V1B9","FTXJ35A2V1BB  / RXJ35M5V1B9","FTXJ35A2V1BB / RXJ35M5V1B9"]
["Dzesēšanas jauda","Nom.","","kW","","","3.50"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","","","428"]
["","EER","","","","","4.09"]
["","COP","","","","","4.04"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","","A"]
["","","Apsilde","","","","A"]
["Apsildes jauda","Nom.","","kW","","","4.00"]
["Notes","","","","","","(1) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","","","(2) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","","","(3) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","","","(4) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["Āra ierīce","","","","RXJ20M5V1B9","RXJ25M5V1B9","","RXJ35M5V1B9"]
["Dzesēšanas jauda","Nom.","","kW","2.30","2.40","","3.50"]
["Apsildes jauda","Nom.","","kW","2.50","3.20","","4.00"]
["Nominālā efektivitāte","EER","","","4.64","4.73","","4.09"]
["","COP","","","5.00","4.57","","4.04"]
["","Gada enerģijas patēriņš","","kWh","248","254","","428"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","A","","A"]
["","","Apsilde","","A","A","","A"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A+++","A+++","","A++"]
["","Jauda","Pdesign","kW","2.30","2.40","","3.50"]
["","SEER","","","8.73","8.64","","7.19"]
["","Gada enerģijas patēriņš","","kWh/a","92","97","","170"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A++","A++","","A++"]
["","Jauda","Pdesign","kW","2.10","2.70","","3.00"]
["","SCOP/A","","","4.61","4.60","","4.60"]
["","Pdh Apsildes jauda pie -10°","","kW","1.80","2.18","","2.61"]
["","Gada enerģijas patēriņš","","kWh/a","638","822","","913"]
["Energy Efficiency Range","","","","A+++ ~ D","A+++ ~ D","","A+++ ~ D"]