{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":5,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXJ-MS / 4MXM-A"]
[]
[]
[]
[]
["","","","","FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / FTXJ20MV1BS / 4MXM80A2V1B"]
["Dzesēšanas jauda","Nom.","","kW","7.50"]
["Telpas dzesēšana","SEER","","","6.92"]
["","Gada enerģijas patēriņš","","kWh/a","380"]
["","Jauda","Pdesign","kW","7.50"]
["","Energoefektivitātes klase","","","A++"]
["Telpu apsilde (mērens klimats)","Jauda","Pdesign","kW","6.46"]
["","SCOP/A","","","4.02"]
["","Energoefektivitātes klase","","","A+"]
["","Gada enerģijas patēriņš","","kWh/a","2,245"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","908"]
["","EER","","","4.13"]
["","COP","","","3.32"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A"]
["","","Apsilde","","C"]
["Apsildes jauda","Nom.","","kW","10.00"]
["Notes","","","","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]