{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":7,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXL-JV"]
[]
[]
[]
[]
["","","","","","FTXL25J2V1B","FTXL35J2V1B"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["","Apsilde","","Nom.","kW","0.040, 0.040, 0.040","0.040, 0.040, 0.040"]
["Korpuss","Krāsa","","","","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","283","283"]
["","","","Platums","mm","770","770"]
["","","","Dziļums","mm","198","198"]
["Svars","Ierīce","","","kg","8.00","8.00"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","9.3","9.3"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","7.7","7.7"]
["","","","Zema","m³/min.","6.1","6.1"]
["","","","Klusa darbība","m³/min.","4.9","4.9"]
["","","Apsilde","Augsta","m³/min.","10.1","10.1"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","8.4","8.4"]
["","","Apsilde","Zema","m³/min.","6.7","6.7"]
["","","","Klusa darbība","m³/min.","5.7","5.7"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","57","57"]
["","Apsilde","","","dBA","57","57"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","41","41"]
["","","","Vidēja","dBA","34","34"]
["","","","Zema","dBA","27","27"]
["","","","Klusa darbība","dBA","23","23"]
["","Apsilde","","Augsta","dBA","41","41"]
["","","","Vidēja","dBA","35","35"]
["","","","Zema","dBA","29","29"]
["","","","Klusa darbība","dBA","26","26"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35"]
["","Gāze","","OD","mm","9.50","9.50"]
["","Aizplūde","","","","18","18"]
["Vadības sistēmas","Infrared remote control","","","","ARC433A87, ARC466A9","ARC433A87, ARC466A9"]
["Standard Accessories","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","2","2"]
["","Batteries","","","","2","2"]
["","Indoor unit fixing screws","","","","2","2"]
["","Mounting plate","","","","1","1"]
["","Remote control holder","","","","1","1"]
["Barošanas avots","Nosaukums","","","","V1","V1"]
["","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]
["Notes","","","","","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V"]