{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":43,"n_cols":6,"rows_kept":43,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXLS-K3"]
[]
[]
[]
[]
["","","","","FTXLS25K3V1B","FTXLS35K3V1B"]
["Skaņas spiediena līmenis","Apsilde","Augsta","dBA","47","47"]
["","","Klusa darbība","dBA","19","19"]
["","","Zema","dBA","23","23"]
["","Dzesēšana","Klusa darbība","dBA","21","21"]
["","","Zema","dBA","33","33"]
["","","Augsta","dBA","45","45"]
["","","Nom.","dBA","37","36"]
["","Dzesēšana","Nom.","dBA","39","39"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","1","1"]
["","Lietošanas rokasgrāmata","","","1","1"]
["","Infrasarkanā tālvadība","","","1","1"]
["","Akumulatori","","","2","2"]
["","Tālvadības turētājs","","","1","1"]
["","Montāžas plāksne","","","1","1"]
["","Titāna apatīta fotokatalītiskais gaisa attīrīšanas filtrs","","","2","2"]
["","Iekštelpu ierīces fiksācijas skrūves","","","2","2"]
["Vadības sistēmas","Infrared remote control","","","ARC466A9","ARC466A9"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35","6.35"]
["","Gāze","OD","mm","9.5","9.5"]
["","Izplūde","","","18","18"]
["Strāvas ievade","Dzesēšana","Nom.","kW","0.024 (2), 0.024 (3), 0.024 (4)","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Apsilde","Nom.","kW","0.030 (2), 0.030 (3), 0.030 (4)","0.030 (2), 0.030 (3), 0.030 (4)"]
["Skaņas jaudas līmenis","Dzesēšana","","dBA","59","59"]
["","Apsilde","","dBA","62","62"]
["Izmēri","Ierīce","Platums","mm","900","900"]
["","","Dziļums","mm","215","215"]
["","","Augstums","mm","298","298"]
["Korpuss","Colour","","","Balts","Balts"]
["Svars","Ierīce","","kg","12","12"]
["Power supply","Phase","","","1~","1~"]
["","Frekvence","","Hz","50","50"]
["","Nosaukums","","","V1","V1"]
["","Spriegums","","V","220-240","220-240"]
["Notes","","","","(1) - Savienojot ar multisistēmas āra ierīci, skatiet pievienojamās āra multiierīces tehniskos datus.","(1) - Savienojot ar multisistēmas āra ierīci, skatiet pievienojamās āra multiierīces tehniskos datus."]
["","","","","(2) - 220 V","(2) - 220 V"]
["","","","","(3) - 230 V","(3) - 230 V"]
["","","","","(4) - 240 V","(4) - 240 V"]