{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":27,"n_cols":11,"rows_kept":27,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXM-R / RZAG-B"]
[]
[]
[]
[]
["","","","","FTXM50R2V1B / RZAG35B5V1B","FTXM35R2V1B / RZAG35B5V1B","FTXM35R5V1B / RZAG35B5V1B","FTXM60R2V1B / RZAG50B5V1B","FTXM50R2V1B / RZAG50B5V1B","FTXM71R2V1B / RZAG60B5V1B","FTXM60R2V1B / RZAG60B5V1B"]
["Dzesēšanas jauda","Min.","","kW","1.6","1.6","1.6","1.7","1.7","1.7","1.7"]
["","Nom.","","kW","3.5","3.5","3.5","5","5","6","6"]
["","Maks.","","kW","5","5","5","6","6","6.8","6.8"]
["Apsildes jauda","Min.","","kW","1.4","1.4","1.4","1.5","1.5","1.6","1.6"]
["","Nom.","","kW","4","4","4","6","6","7","7"]
["","Maks.","","kW","5.3","5.3","5.3","6.5","6.5","7.5","7.5"]
["Nominālā efektivitāte","EER","","","4.32","4.3","4.3","4.04","4","3.5","3.5"]
["","COP","","","3.93","3.85","3.85","4.08","4","3.68","3.61"]
["","Gada enerģijas patēriņš","","kWh","405","407","407","619","625","857","857"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","A","A","A","A","A","A"]
["","","Apsilde","","A","A","A","A","A","A","A"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A++","A++","A++","A++","A++","A++","A++"]
["","Jauda","Pdesign","kW","3.5","3.5","3.5","5","5","6","6"]
["","SEER","","","7.76","7.7","7.7","7.53","7.41","6.9","6.9"]
["","Gada enerģijas patēriņš","","kWh/a","158","159","159","232","236","304","304"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A++","A++","A++","A++","A++","A+","A+"]
["","Jauda","Pdesign","kW","2.6","2.6","2.6","4.5","4.5","4.5","4.6"]
["","SCOP/A","","","4.68","4.6","4.6","4.69","4.6","4.4","4.35"]
["","Pdh Apsildes jauda pie -10°","","kW","2.47","2.47","2.47","3.89","3.89","3.95","4.02"]
["","Gada enerģijas patēriņš","","kWh/a","778","790","790","1344","1369","1433","1480"]
["Energoefektivitātes diapazons","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D","A+++ ~ D"]