{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":33,"n_cols":6,"rows_kept":33,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-M9 / 2MXM-A9"]
[]
[]
[]
[]
["","","","","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM40A2V1B9","FTXP20M5V1B9 / FTXP20M5V1B9 / 2MXM50A2V1B9"]
["Dzesēšanas jauda","Nom.","","kW","4"]
["Apsildes jauda","Nom.","","kW","4.2"]
["Nominālā efektivitāte","EER","","","3.71"]
["","COP","","","3.75"]
["","Gada enerģijas patēriņš","","kWh","539"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A"]
["","","Apsilde","","A"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A++"]
["","Jauda","Pdesign","kW","4"]
["","SEER","","","7.74"]
["","Gada enerģijas patēriņš","","kWh/a","181"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A+"]
["","Jauda","Pdesign","kW","3.2"]
["","SCOP/A","","","4.3"]
["","Pdh Apsildes jauda pie -10°","","kW","2.46"]
["","Gada enerģijas patēriņš","","kWh/a","1041"]
["Notes","","","","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(1) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temperatūru: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(2) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["","","","","(3) - Darbības diapazonu skatiet atsevišķā attēlā","(3) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(4) - Elektrības datus skatiet atsevišķā zīmējumā","(4) - Elektrības datus skatiet atsevišķā zīmējumā"]
["Dzesēšanas jauda","Nom.","","kW","","4.00"]
["Apsildes jauda","Nom.","","kW","","5.20"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","","554"]
["","COP","","","","3.68"]
["","EER","","","","3.61"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","","A"]
["","","Apsilde","","","A"]