{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":7,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXP-N9 / RXP-M"]
[]
[]
[]
[]
["","","","","FTXP20N5V1B9 / RXP20M5V1B","FTXP25N5V1B9 / RXP25M5V1B","FTXP35N5V1B9 / RXP35M5V1B"]
["Āra ierīce","","","","RXP20M5V1B","RXP25M5V1B","RXP35M5V1B"]
["Dzesēšanas jauda","Min.","","kW","1.3","1.3","1.3"]
["","Nom.","","kW","2","2.5","3.5"]
["","Maks.","","kW","2.6","3","4"]
["Apsildes jauda","Min.","","kW","1.3","1.3","1.3"]
["","Nom.","","kW","2.5","3","4"]
["","Maks.","","kW","3.5","4","4.8"]
["Nominālā efektivitāte","EER","","","3.75","3.75","3.48"]
["","COP","","","4.77","4.36","4.02"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","A","A"]
["","","Apsilde","","A","A","A"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A++","A++","A++"]
["","Jauda","Pdesign","kW","2","2.5","3.5"]
["","SEER","","","7.2","7.2","7.2"]
["","Gada enerģijas patēriņš","","kWh/a","97","121","170"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A++","A++","A++"]
["","Jauda","Pdesign","kW","2.2","2.4","2.8"]
["","SCOP/A","","","4.65","4.61","4.64"]
["","Pdh Apsildes jauda pie -10°","","kW","1.99","2.09","2.35"]
["","Gada enerģijas patēriņš","","kWh/a","663","728","845"]
["Energoefektivitātes diapazons","","","","A+++ ~ D","A+++ ~ D","A+++ ~ D"]
["Notes","","","","(1) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(1) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m.","(1) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]
["","","","","(2) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(2) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m.","(2) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā","(3) - Elektrības datus skatiet atsevišķā zīmējumā","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]