{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":18,"n_cols":6,"rows_kept":18,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RKS-F"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RKS60F3V1B","FTXS71GV1B / RKS71FAV1B"]
["Dzesēšanas jauda","Min.","","kW","1.7","2.3"]
["","Maks.","","kW","6.7","8.5"]
["","Nom.","","kW","6.0 (1)","7.1 (1)"]
["Cauruļvadu savienojumi","Šķidrums","OD","mm","6.35","6.35"]
["","Gāze","OD","mm","12.7","15.9"]
["","Izplūde","OD","mm","18.0","18.0"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","995","1,175"]
["","EER","","","3.02","3.02"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","B","D"]
["Notes","","","","(1) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m","(1) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m"]
["","","","","(2) - Jaudas ir neto, neiekļaujot dzesēšanas atskaitījumu iekštelpu ventilatora motora siltumam.","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]
["","","","","(3) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]