{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":31,"n_cols":5,"rows_kept":31,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G / RXS-L"]
[]
[]
[]
[]
["","","","","FTXS60GV1B / RXS60L2V1B"]
["Dzesēšanas jauda","Min.","","kW","1.7"]
["","Nom.","","kW","6.0"]
["","Maks.","","kW","6.7"]
["Apsildes jauda","Min.","","kW","1.7"]
["","Nom.","","kW","7.0"]
["","Maks.","","kW","8.0"]
["Nominālā efektivitāte","EER","","","3.02"]
["","COP","","","3.43"]
["","Gada enerģijas patēriņš","","kWh","995"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","B"]
["","","Apsilde","","B"]
["Cauruļvadu savienojumi","Izplūde","OD","mm","18"]
["Cauruļu savienojumi","Gāze","OD","mm","12.7"]
["","Šķidrums","OD","mm","6.35"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A"]
["","Jauda","Pdesign","kW","6.00"]
["","SEER","","","5.58"]
["","Gada enerģijas patēriņš","","kWh/a","376"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A"]
["","Jauda","Pdesign","kW","4.80"]
["","SCOP/A","","","3.89"]
["","Gada enerģijas patēriņš","","kWh/a","1728"]
["Notes","","","","(1) - 220 V"]
["","","","","(2) - 230V"]
["","","","","(3) - 240V"]