{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":85,"n_cols":12,"rows_kept":85,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-G"]
[]
[]
[]
[]
["","","","","","FTXS20G2V1B","FTXS25G2V1B","FTXS35G2V1B","FTXS42G2V1B","FTXS50G2V1B","FTXS60GV1B","FTXS71GV1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","38","39","42","42","44","","46"]
["","","","Klusa darbība","dBA","25","25","26","30","31","","34"]
["","","","Zema","dBA","28","28","29","33","34","","37"]
["","Dzesēšana","","Klusa darbība","dBA","22","22","23","30","31","","34"]
["","","","Zema","dBA","25","25","26","33","34","","37"]
["","","","Augsta","dBA","38","38","42","42","43","","46"]
["","","","Nom.","dBA","33","34","36","38","39","","42"]
["","Dzesēšana","","Nom.","dBA","32","32","34","38","39","","42"]
["Standard Accessories","Titāna apatīta fotokatalītiskais gaisa attīrīšanas filtrs","","","","2","2","2","2","2"]
["","Lietošanas rokasgrāmata","","","","1","1","1","1","1","","1"]
["","Uzstādīšanas rokasgrāmata","","","","1","1","1","1","1","","1"]
["","Bezvadu tālvadības pults","","","","1","1","1","1","1","","1"]
["","Akumulatori","","","","2","2","2","2","2","","2"]
["","Tālvadības turētājs","","","","1","1","1","1","1","","1"]
["","Iekštelpu ierīces fiksācijas skrūves","","","","2","2","2","2","2","","2"]
["","Montāžas plāksne","","","","1","1","1","1","1","","1"]
["Vadības sistēmas","Infrared remote control","","","","","","","","","","ARC452A3"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35","6.35","6.35","6.35","","6.35"]
["","Gāze","","OD","mm","9.52","9.52","9.52","9.52","12.70","","15.9"]
["","Izplūde","","","","18","18","18","18","18","","18"]
["Power input","Dzesēšana","","Nom.","kW","","","","","","","0.045 (2), 0.045 (3), 0.045 (4)"]
["","Apsilde","","Nom.","kW","","","","","","","0.060 (2), 0.060 (3), 0.060 (4)"]
["Sound power level","Dzesēšana","","","dBA","54","54","58","58","59","","63"]
["","Apsilde","","","dBA","54","55","58","58","60","","62"]
["Izmēri","Ierīce","","Platums","mm","800","800","800","800","800","","1,050"]
["","","","Dziļums","mm","215","215","215","215","215","","250"]
["","","","Augstums","mm","295","295","295","295","295","","290"]
["Korpuss","Krāsa","","","","Balts","Balts","Balts","Balts","Balts","","Balts"]
["Svars","Ierīce","","","kg","9","9","10","10","10","","12"]
["Power supply","Fāze","","","","1~","1~","1~","1~","1~","","1~"]
["","Frekvence","","","Hz","50","50","50","50","50","","50"]
["","Nosaukums","","","","V1","V1","V1","V1","V1","","V1"]
["","Spriegums","","","V","220-240","220-240","220-240","220-240","220-240","","220-240"]
["Notes","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - SL: gaisa plūsmas ātruma iestatījuma klusais ventilatora līmenis"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Nom.","m³/min.","","","","","","16.0"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","","","","","","41"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Nom.","m³/min.","","","","","","14.9"]
["Skaņas spiediena līmenis","Apsilde","","Nom.","dBA","","","","","","40"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","","","","","","0.040 (4) (2) (3), 0.040 (4) (2) (3), 0.040 (4) (2) (3)"]
["","Apsilde","","Nom.","kW","","","","","","0.045 (4) (2) (3), 0.045 (4) (2) (3), 0.045 (4) (2) (3)"]
["Korpuss","Krāsa","","","","","","","","","Balts"]
["Izmēri","Ierīce","","Augstums","mm","","","","","","290"]
["","","","Platums","mm","","","","","","1050"]
["","","","Dziļums","mm","","","","","","250"]
["Svars","Ierīce","","","kg","","","","","","12"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","","","","","16.0"]
["","","","Zema","m³/min.","","","","","","11.3"]
["","","","Klusa darbība","m³/min.","","","","","","10.1"]
["","","Apsilde","Augsta","m³/min.","","","","","","17.2"]
["","","","Zema","m³/min.","","","","","","12.6"]
["","","","Klusa darbība","m³/min.","","","","","","11.3"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","","","","","60"]
["","Apsilde","","","dBA","","","","","","59"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","","","","","45"]
["","","","Zema","dBA","","","","","","36"]
["","","","Klusa darbība","dBA","","","","","","33"]
["","Apsilde","","Augsta","dBA","","","","","","44"]
["","","","Zema","dBA","","","","","","35"]
["","","","Klusa darbība","dBA","","","","","","32"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","","","","","6.35"]
["","Gāze","","OD","mm","","","","","","12.7"]
["","Aizplūde","","","","","","","","","18"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","","","","","","ARC452A3"]
["Standard Accessories","Installation manual","","","","","","","","","1"]
["","Wireless remote control","","","","","","","","","1"]
["","Operation manual","","","","","","","","","1"]
["","Batteries","","","","","","","","","2"]
["","Indoor unit fixing screws","","","","","","","","","2"]
["","Mounting plate","","","","","","","","","1"]
["","Remote control holder","","","","","","","","","1"]
["","Titanium apatite photocatalytic air purification filter","","","","","","","","","2"]
["Barošanas avots","Nosaukums","","","","","","","","","V1"]
["","Fāze","","","","","","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","","","","","","50"]
["","Spriegums","","","V","","","","","","220-240"]
["Standard Accessories","Titāna apatīta fotokatalītiskais gaisa attīrīšanas filtrs bez rāmja","","","","","","","","","","2"]
["Notes","","","","","","","","","","","(4) - 240 V"]