{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":25,"n_cols":10,"rows_kept":25,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K / RXS-L3"]
[]
[]
[]
[]
["","","","","FTXS20K3V1B / RXS20L3V1B","FTXS20K2V1B / RXS20L3V1B","FTXS25K3V1B / RXS25L3V1B","FTXS25K2V1B / RXS25L3V1B","FTXS35K2V1B / RXS35L3V1B","FTXS35K3V1B / RXS35L3V1B"]
["Dzesēšanas jauda","Min.","","kW","","","","","","1.4"]
["","Maks.","","kW","","","","","","4.0"]
["","Nom.","","kW","2.00 (2)","2.0","2.5 (2)","2.5","3.5","3.5 (2)"]
["Cauruļu savienojumi","Šķidrums","OD","mm","6.35","","6.35","","","6.35"]
["","Gāze","OD","mm","9.5","","9.5","","","9.5"]
["","Aizplūde","OD","mm","18","","18","","","18"]
["Nominālā efektivitāte","Gada enerģijas patēriņš","","kWh","228","228","297","297","450","450"]
["","EER","","","4.39 (1)","4.39","4.21 (1)","4.21","3.89","3.89 (1)"]
["","COP","","","4.72 (1)","4.72","4.67 (1)","4.67","4.76","4.76 (1)"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A","A","A","A","A","A"]
["","","Apsilde","","A","A","A","A","A","A"]
["Apsildes jauda","Nom.","","kW","2.5 (2)","2.5","2.8 (2)","2.8","4.0","4.00 (2)"]
["","Min.","","kW","1.3","","1.3","","","1.4"]
["","Maks.","","kW","4.3","","4.7","","","5.2"]
["Notes","","","","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES","(1) - EER/COP saskaņā ar Eurovent 2012, lietošanai vienīgi ārpus ES"]
["","","","","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda","(2) - Nominālā efektivitāte: dzesēšana pie 35°/27° nominālā jauda, apsilde pie 7°/20° nominālā jauda"]
["","","","","(3) - 220 V","","(3) - 220 V","","","(3) - 220 V"]
["","","","","(4) - 230 V","","(4) - 230 V","","","(4) - 230 V"]
["","","","","(5) - 240 V","","(5) - 240 V","","","(5) - 240 V"]