{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":91,"n_cols":15,"rows_kept":91,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXS-K"]
[]
[]
[]
[]
["","","","","","FTXS20K2V1B","FTXS20K3V1B","FTXS25K2V1B","FTXS25K3V1B","FTXS35K2V1B","FTXS35K3V1B","FTXS42K2V1B","FTXS42K3V1B","FTXS50K2V1B","FTXS50K3V1B"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","40","","","","","","45"]
["","","","Klusa darbība","dBA","19","","","","","","22"]
["","","","Zema","dBA","27","","","","","","33"]
["","Dzesēšana","","Klusa darbība","dBA","19","","","","","","21"]
["","","","Zema","dBA","24","","","","","","33"]
["","","","Augsta","dBA","40","","","","","","45"]
["","","","Nom.","dBA","34","","","","","","39"]
["","Dzesēšana","","Nom.","dBA","32","","","","","","39"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1","","","","","","1"]
["","Lietošanas rokasgrāmata","","","","1","","","","","","1"]
["","Bezvadu tālvadības pults","","","","1","","","","","","1"]
["","Akumulatori","","","","2","","","","","","2"]
["","Tālvadības turētājs","","","","1","","","","","","1"]
["","Montāžas plāksne","","","","1","","","","","","1"]
["","Iekštelpu ierīces fiksācijas skrūves","","","","2","","","","","","2"]
["","Titāna apatīta fotokatalītiskais gaisa attīrīšanas filtrs","","","","2","","","","","","2"]
["Control systems","Infrared remote control","","","","ARC466A6","","","","","","ARC466A6"]
["Cauruļvadu savienojumi","Šķidrums","","OD","mm","6.35","","","","","","6.35"]
["","Gas","","OD","mm","9.5","","","","","","9.5"]
["","Izplūde","","","","18","","","","","","18"]
["Jaudas izlietojums","Dzesēšana","","Nom.","kW","0.04","","","","","","0.024 (2), 0.024 (3), 0.024 (4)"]
["","Apsilde","","Nom.","kW","0.04","","","","","","0.030 (2), 0.030 (3), 0.030 (4)"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","58","","","","","","59"]
["","Apsilde","","","dBA","58","","","","","","59"]
["Izmēri","Ierīce","","Platums","mm","780","","","","","","900"]
["","","","Dziļums","mm","215","","","","","","215"]
["","","","Augstums","mm","289","","","","","","298"]
["Casing","Krāsa","","","","Balts","","","","","","Balts"]
["Svars","Ierīce","","","kg","8","","","","","","11"]
["Power supply","Fāze","","","","1~","","","","","","1~"]
["","Frekvence","","","Hz","50","","","","","","50"]
["","Name","","","","V1","","","","","","V1"]
["","Spriegums","","","V","220-240","","","","","","220-240"]
["Notes","","","","","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - 220 V","(1) - Savienojot ar multisistēmas āra ierīci, skatiet pievienojamās āra multiierīces tehniskos datus.","(1) - 220 V","(1) - 220 V","(1) - 220 V"]
["","","","","","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 230 V","(2) - 220 V","(2) - 230 V","(2) - 230 V","(2) - 230 V"]
["","","","","","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 240 V","(3) - 230 V","(3) - 240 V","(3) - 240 V","(3) - 240 V"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (3) (1) (2), 0.040 (3) (1) (2), 0.040 (3) (1) (2)","0.026 (3) (4) (2), 0.026 (3) (4) (2), 0.026 (3) (4) (2)","0.026 (1) (3) (2), 0.026 (1) (3) (2), 0.026 (1) (3) (2)","","0.024, 0.024, 0.024","0.026 (4) (2) (3), 0.026 (4) (2) (3), 0.026 (4) (2) (3)","0.026 (1) (2) (3), 0.026 (1) (2) (3), 0.026 (1) (2) (3)"]
["","Apsilde","","Nom.","kW","","0.040, 0.040, 0.040","0.04","0.040 (2) (3) (1), 0.040 (2) (3) (1), 0.040 (2) (3) (1)","0.028 (2) (4) (3), 0.028 (2) (4) (3), 0.028 (2) (4) (3)","0.028 (1) (3) (2), 0.028 (1) (3) (2), 0.028 (1) (3) (2)","","0.030, 0.030, 0.030","0.032 (2) (4) (3), 0.032 (2) (4) (3), 0.032 (2) (4) (3)","0.032 (2) (1) (3), 0.032 (2) (1) (3), 0.032 (2) (1) (3)"]
["Korpuss","Krāsa","","","","","Balts","Balts","Balts","Balts","Balts","","Balts","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","","215","289","215","298","215","","215","298","215"]
["","","","Platums","mm","","780","780","780","900","900","","900","900","900"]
["","","","Dziļums","mm","","289","215","289","215","298","","298","215","298"]
["Svars","Ierīce","","","kg","","8.00","8","8.00","11","11.0","","11.0","11","11.0"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","","8.8","9.1","9.1","11.2","11.2","","11.2","11.9","11.9"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","","6.7","7.0","7.0","","8.5","","9.1","","9.6"]
["","","","Zema","m³/min.","","4.7","5.0","5.0","5.8","5.8","","7.0","7.4","7.4"]
["","","","Klusa darbība","m³/min.","","3.9","3.9","3.9","4.1","4.1","","4.1","4.5","4.5"]
["","","Apsilde","Augsta","m³/min.","","9.5","10.0","10.0","12.1","12.1","","12.4","13.3","13.3"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","","7.8","8.0","8.0","","9.3","","10.0","","10.8"]
["","","Apsilde","Zema","m³/min.","","6.0","6.0","6.0","6.5","6.5","","7.8","8.4","8.4"]
["","","","Klusa darbība","m³/min.","","4.3","4.3","4.3","4.2","4.2","","5.2","5.5","5.5"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","","58","58","58","59","59","","59","60","60"]
["","Apsilde","","","dBA","","58","58","58","59","59","","59","60","60"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","","40","41","41","45","45","","45","46","46"]
["","","","Vidēja","dBA","","32","33","33","","37","","39","","40"]
["","","","Zema","dBA","","24","25","25","29","29","","33","34","34"]
["","","","Klusa darbība","dBA","","19","19","19","19","19","","21","23","23"]
["","Apsilde","","Augsta","dBA","","40","41","41","45","45","","45","47","47"]
["","","","Vidēja","dBA","","34","34","34","","39","","39","","40"]
["","","","Zema","dBA","","27","27","27","29","29","","33","34","34"]
["","","","Klusa darbība","dBA","","19","19","19","19","19","","22","24","24"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","","6.35","6.35","6.35","6.35","6.35","","6.35","6.35","6.35"]
["","Gāze","","OD","mm","","9.50","9.5","9.50","9.5","9.50","","9.50","12.7","12.7"]
["","Aizplūde","","","","","18","18","18","18","18","","18","18","18"]
["Control systems","Infrared remote control","","","","","ARC466A6","","","","","","ARC466A9"]
["Standard Accessories","Installation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Wireless remote control","","","","","1","1","1","1","1","","1","1","1"]
["","AAA dry-cell batteries","","","","","2","","2","","2","","2","","2"]
["","Operation manual","","","","","1","1","1","1","1","","1","1","1"]
["","Titanium apatite deodorizing filter","","","","","2","","2","","2","","2","","2"]
["","Indoor unit fixing screws","","","","","2","2","2","2","2","","2","2","2"]
["","Mounting plate","","","","","1","1","1","1","1","","1","1","1"]
["","Remote control holder","","","","","1","1","1","1","1","","1","1","1"]
["Barošanas avots","Nosaukums","","","","","V1","V1","V1","V1","V1","","V1","V1","V1"]
["","Fāze","","","","","1~","1~","1~","1~","1~","","1~","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","","50","50","50","50","50","","50","50","50"]
["","Spriegums","","","V","","220-240","220-240","220-240","220-240","220-240","","220-240","220-240","220-240"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Nom.","m³/min.","","","9.1","","11.2","","","","11.9"]
["Skaņas spiediena līmenis","Dzesēšana","","Nom.","dBA","","","33","","37","","","","40"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Nom.","m³/min.","","","8.0","","9.3","","","","10.8"]
["Skaņas spiediena līmenis","Apsilde","","Nom.","dBA","","","34","","39","","","","40"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","","","ARC466A6","ARC466A6","ARC466A6","ARC466A9","","","ARC466A6","ARC466A9"]
["Standard Accessories","Batteries","","","","","","2","","2","","","","2"]
["","Titanium apatite photocatalytic air purification filter","","","","","","2","","2","","","","2"]
["Notes","","","","","","","","","","","(4) - 240 V"]