{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":53,"n_cols":6,"rows_kept":53,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-BB"]
[]
[]
[]
[]
["","","","","","FTXTA30B2V1BB"]
["Skaņas spiediena līmenis","Apsilde","","Augsta","dBA","41"]
["","","","Vidēja","dBA","31"]
["","","","Klusa darbība","dBA","19"]
["","","","Zema","dBA","24"]
["","Dzesēšana","","Vidēja","dBA","32"]
["","","","Klusa darbība","dBA","20"]
["","","","Zema","dBA","25"]
["","","","Augsta","dBA","43"]
["Standard Accessories","Uzstādīšanas rokasgrāmata","","","","1"]
["","Lietošanas rokasgrāmata","","","","1"]
["","Gaisa filtrs","","","","2"]
["","Infrasarkanā tālvadība","","","","1"]
["","Attālā kontrollera montāžas plāksne","","","","1"]
["","Skrūvju somiņa","","","","1"]
["","Skrūvju pārsegs","","","","2"]
["","AAA sausās baterijas","","","","2"]
["","Vispārēji drošības pasākumi","","","","1"]
["Refrigerant","GWP","","","","675.0"]
["Vadības sistēmas","Wired remote control","","","","BRC073A4"]
["","Infrared remote control","","","","ARC466A59"]
["Piping connections","Šķidrums","","OD","mm","6.35"]
["","Gāze","","OD","mm","9.50"]
["","Izplūde","","","","18"]
["Jaudas izlietojums","Dzesēšana","","Nom.","kW","0.023"]
["","Apsilde","","Nom.","kW","0.022"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","60"]
["","Apsilde","","","dBA","60"]
["Izmēri","Ierīce","","Platums","mm","798"]
["","","","Dziļums","mm","189"]
["","","","Augstums","mm","295"]
["Korpuss","Colour","","","","Melns"]
["Svars","Ierīce","","","kg","11.5"]
["Ventilators","Gaisa plūsmas ātrums","Apsilde","Augsta","m³/min.","11.5"]
["","","","Zema","m³/min.","6.0"]
["","","","Vidēja","m³/min.","8.0"]
["","","","Klusa darbība","m³/min.","5.1"]
["","","Dzesēšana","Zema","m³/min.","5.7"]
["","","","Vidēja","m³/min.","8.3"]
["","","","Augsta","m³/min.","11.9"]
["","","","Klusa darbība","m³/min.","4.6"]
["Power supply","Phase","","","","1~"]
["","Frekvence","","","Hz","50"]
["","Nosaukums","","","","V1"]
["","Spriegums","","","V","220-240"]
["Notes","","","","","(1) - Dzesēšana: iekšējā temp. 27 °CDB,19,0 °CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m"]
["","","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m"]
["","","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]