{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":30,"n_cols":5,"rows_kept":30,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CW / RXTA-C"]
[]
[]
[]
[]
["","","","","FTXTA30C2V1BW / RXTA30C2V1B"]
["Dzesēšanas jauda","Min.","","kW","1.2"]
["","Nom.","","kW","3"]
["","Maks.","","kW","4.6"]
["Apsildes jauda","Min.","","kW","0.8"]
["","Nom.","","kW","3.2"]
["","Maks.","","kW","7.1"]
["Nominālā efektivitāte","EER","","","4.89"]
["","COP","","","5.01"]
["","Gada enerģijas patēriņš","","kWh","307"]
["","Enerģijas marķēšanas direktīva","Dzesēšana","","A"]
["","","Apsilde","","A"]
["Telpu dzesēšana","Energoefektivitātes klase","","","A+++"]
["","Jauda","Pdesign","kW","3"]
["","SEER","","","8.75"]
["","Gada enerģijas patēriņš","","kWh/a","120"]
["Telpu apsilde (mērens klimats)","Energoefektivitātes klase","","","A+++"]
["","Jauda","Pdesign","kW","3"]
["","SCOP/A","","","5.17"]
["","Pdh Apsildes jauda pie -10°","","kW","3"]
["","Gada enerģijas patēriņš","","kWh/a","812"]
["Notes","","","","(1) - Elektrības datus skatiet atsevišķā zīmējumā"]
["","","","","(2) - Darbības diapazonu skatiet atsevišķā attēlā"]
["","","","","(3) - Nominālā dzesēšanas jauda noteikta, pamatojoties uz: iekštelpu temp.: 27°CDB, 19°CWB, āra temperatūru: 35°CDB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m, līmeņa atšķirība: 0 m."]
["","","","","(4) - Nominālās apsildes jaudas balstās uz: iekštelpas temperatūru: 20°CDB, ārējo temperatūru: 7°CDB, 6°CWB, ekvivalentā dzesētāja cauruļvadu sistēma: 5m, līmeņa atšķirība: 0 m."]