{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":50,"n_cols":6,"rows_kept":50,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTA-CW"]
[]
[]
[]
[]
["","","","","","FTXTA30C2V1BW"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.023"]
["","Apsilde","","Nom.","kW","0.022"]
["Korpuss","Krāsa","","","","Balts"]
["Izmēri","Ierīce","","Augstums","mm","295"]
["","","","Platums","mm","798"]
["","","","Dziļums","mm","189"]
["Svars","Ierīce","","","kg","12"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","13.1"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","9"]
["","","","Zema","m³/min.","6"]
["","","","Klusa darbība","m³/min.","4.9"]
["","","Apsilde","Augsta","m³/min.","12.3"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","8.2"]
["","","Apsilde","Zema","m³/min.","5.8"]
["","","","Klusa darbība","m³/min.","5"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","60"]
["","Apsilde","","","dBA","60"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","43"]
["","","","Vidēja","dBA","32"]
["","","","Zema","dBA","25"]
["","","","Klusa darbība","dBA","20"]
["","Apsilde","","Augsta","dBA","41"]
["","","","Vidēja","dBA","31"]
["","","","Zema","dBA","24"]
["","","","Klusa darbība","dBA","19"]
["Aukstumaģents","GWP","","","","675"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35"]
["","Gāze","","OD","mm","9.5"]
["","Aizplūde","","","","18"]
["Control systems","Infrared remote control","","","","ARC466A84"]
["Vadības sistēmas","Tālv. pults ar vadu","","","","BRC073A4"]
["Standard Accessories","Installation manual","","","","1"]
["","Wireless remote control","","","","1"]
["","Screw cover","","","","2"]
["","AAA dry-cell batteries","","","","2"]
["","General safety precautions","","","","1"]
["","Operation manual","","","","1"]
["","Titanium apatite deodorizing filter","","","","1"]
["","Silver particle filter","","","","1"]
["","Remote control holder","","","","1"]
["","Screw bag","","","","1"]
["Barošanas avots","Fāze","","","","1~"]
["Strāvas padeve","Frekvence","","","Hz","50"]
["","Spriegums","","","V","220-240"]