{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":55,"n_cols":7,"rows_kept":55,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-A"]
[]
[]
[]
[]
["","","","","","FTXTM30A2V1B","FTXTM40A2V1B"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.029","0.053"]
["","Apsilde","","Nom.","kW","0.024","0.06"]
["Korpuss","Krāsa","","","","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","298","298"]
["","","","Platums","mm","804","997"]
["","","","Dziļums","mm","252","292"]
["Svars","Ierīce","","","kg","12","15"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","13.2","15.1"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","8.1","9.2"]
["","","","Zema","m³/min.","5.6","5.6"]
["","","","Klusa darbība","m³/min.","4.8","4.8"]
["","","Apsilde","Augsta","m³/min.","11.7","17"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","7.7","10"]
["","","Apsilde","Zema","m³/min.","5.6","6"]
["","","","Klusa darbība","m³/min.","4.7","5.1"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","60","60"]
["","Apsilde","","","dBA","59","60"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","45","46"]
["","","","Vidēja","dBA","33","32"]
["","","","Zema","dBA","25","24"]
["","","","Klusa darbība","dBA","21","20"]
["","Apsilde","","Augsta","dBA","43","46"]
["","","","Vidēja","dBA","31","31"]
["","","","Zema","dBA","22","22"]
["","","","Klusa darbība","dBA","19","19"]
["Aukstumaģents","GWP","","","","675","675"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35"]
["","Gāze","","OD","mm","9.5","9.5"]
["","Aizplūde","","","","18","18"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","ARC466A83","ARC466A83"]
["Standard Accessories","FTXTM30A2V1B","","","","1"]
["","Installation manual","","","","1","1"]
["","Wireless remote control","","","","1","1"]
["","Screw cover","","","","2","2"]
["","AAA dry-cell batteries","","","","2","2"]
["","General safety precautions","","","","1","1"]
["","Operation manual","","","","1","1"]
["","Titanium apatite deodorizing filter","","","","1","1"]
["","Silver particle filter","","","","1","1"]
["","Remote control holder","","","","1","1"]
["","Screw bag","","","","1","1"]
["Barošanas avots","Nosaukums","","","","V1","V1"]
["","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]
["Notes","","","","","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m","(1) - Dzesēšana: iekšējā temp. 27°CDB, 19°CWB; ārējā temp. 35 °CDB, 24 °CWB; ekvivalentais cauruļvadu garums: 5 m"]
["","","","","","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m","(2) - Apsilde: iekšējā temp. 20 °CDB; ārējā temp. 7 °CDB, 6 °CWB; ekvivalentā dzesēšanas cauruļvadu sistēma: 5 m"]
["","","","","","(3) - Elektrības datus skatiet atsevišķā zīmējumā","(3) - Elektrības datus skatiet atsevišķā zīmējumā"]
["Standard Accessories","FTXTM40A2V1B","","","","","1"]