{"text_format":"2","workbook":"xls","n_sheets":1,"sheets":["Products"],"not_rendered":{"charts":0,"images":0,"macros":0,"external_links":1,"defined_names":0,"comments":0,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"run_cost":"one","rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900","formulas":"cached_only"}

{"sheet":"Products","index":0,"n_rows":40,"n_cols":7,"rows_kept":40,"cut":false,"hidden":false,"merged":[],"flags":["formulas_cached_only"]}
["PRODUCT NAME","FTXTM-M"]
[]
[]
[]
[]
["","","","","","FTXTM30M2V1B","FTXTM40M2V1B"]
["Strāvas ievade","Dzesēšana","","Nom.","kW","0.032","0.037"]
["","Apsilde","","Nom.","kW","0.037","0.04"]
["Korpuss","Krāsa","","","","Balts","Balts"]
["Izmēri","Ierīce","","Augstums","mm","294","300"]
["","","","Platums","mm","811","1040"]
["","","","Dziļums","mm","272","295"]
["Svars","Ierīce","","","kg","10","14.5"]
["Ventilators","Gaisa plūsmas ātrums","Dzesēšana","Augsta","m³/min.","11.7","15.5"]
["","Gaisa caurplūde","Dzesēšana","Vidēja","m³/min.","8","9.2"]
["","","","Zema","m³/min.","6.3","5.7"]
["","","","Klusa darbība","m³/min.","5.2","4.6"]
["","","Apsilde","Augsta","m³/min.","12.2","17.7"]
["","Gaisa caurplūde","Apsilde","Vidēja","m³/min.","7.5","11"]
["","","Apsilde","Zema","m³/min.","5.1","7.5"]
["","","","Klusa darbība","m³/min.","4.1","6.3"]
["Skaņas jaudas līmenis","Dzesēšana","","","dBA","60","60"]
["","Apsilde","","","dBA","61","61"]
["Skaņas spiediena līmenis","Dzesēšana","","Augsta","dBA","45","46"]
["","","","Vidēja","dBA","33","32"]
["","","","Zema","dBA","25","24"]
["","","","Klusa darbība","dBA","21","20"]
["","Apsilde","","Augsta","dBA","45","46"]
["","","","Vidēja","dBA","31","31"]
["","","","Zema","dBA","22","22"]
["","","","Klusa darbība","dBA","19","19"]
["Cauruļu savienojumi","Šķidrums","","OD","mm","6.35","6.35"]
["","Gāze","","OD","mm","9.5","9.5"]
["","Aizplūde","","","","16 (pievienošanas šļūtenes iekšējais diametrs)","16 (pievienošanas šļūtenes iekšējais diametrs)"]
["Vadības sistēmas","Infrasarkano staru tālv. pults","","","","ARC466A55","ARC466A55"]
["","Tālv. pults ar vadu","","","","BRC944B2, BRC073A1","BRC944B2, BRC073A1"]
["Barošanas avots","Nosaukums","","","","V1","V1"]
["","Fāze","","","","1~","1~"]
["Strāvas padeve","Frekvence","","","Hz","50","50"]
["","Spriegums","","","V","220-240","220-240"]